X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/GMRES2stage.git/blobdiff_plain/23054d081ea510f87cf5c9d8ed9351034ffa8f45..dfdee1f9086e9574b81e615edd998441ed3b82ae:/paper.tex

diff --git a/paper.tex b/paper.tex
index c183ea4..c8305c5 100644
--- a/paper.tex
+++ b/paper.tex
@@ -611,19 +611,19 @@ equations arising from very large and complex problems.
 GMRES is one of the most  widely used Krylov iterative method for solving sparse
 and large  linear systems. It  has been developed by  Saad \emph{et al.}~\cite{Saad86}  as a
 generalized  method to  deal with  unsymmetric and  non-Hermitian  problems, and
-indefinite symmetric problems too. In its original version called full GMRES, it
+indefinite symmetric problems too. In its original version called full GMRES, this algorithm
 minimizes the residual over the  current Krylov subspace until convergence in at
-most $n$ iterations,  where $n$ is the  size of the sparse matrix.  It should be
-noticed that full GMRES is too expensive in the case of large matrices since the
+most $n$ iterations,  where $n$ is the  size of the sparse matrix.  
+Full GMRES is however too much expensive in the case of large matrices, since the
 required orthogonalization  process per  iteration grows quadratically  with the
-number of iterations. For that reason, in practice GMRES is restarted after each
-$m\ll n$ iterations to avoid the  storage of a large orthonormal basis. However,
+number of iterations. For that reason, GMRES is restarted in practice after each
+$m\ll n$ iterations, to avoid the  storage of a large orthonormal basis. However,
 the  convergence behavior  of the  restarted GMRES,  called GMRES($m$),  in many
-cases depends quite critically on  the value of $m$~\cite{Huang89}. Therefore in
+cases depends quite critically on  the $m$ value~\cite{Huang89}. Therefore in
 most cases, a preconditioning technique is applied to the restarted GMRES method
 in order to improve its convergence.
 
-In order to enhance the robustness of Krylov iterative solvers, some techniques have been proposed allowing the use of different preconditioners, if necessary, within the iteration instead of restarting. Those techniques may lead to considerable savings in CPU time and memory requirements. Van der Vorst in~\cite{Vorst94} has proposed variants of the GMRES algorithm in which a different preconditioner is applied in each iteration, so-called GMRESR family of nested methods. In fact, the GMRES method is effectively preconditioned with other iterative schemes (or GMRES itself), where the iterations of the GMRES method are called outer iterations while the iterations of the preconditioning process referred to as inner iterations. Saad in~\cite{Saad:1993} has proposed FGMRES which is another variant of the GMRES algorithm using a variable preconditioner. In FGMRES the search directions are preconditioned whereas in GMRESR the residuals are preconditioned. However in practice the good preconditioners are those based on direct methods, as ILU preconditioners, which are not easy to parallelize and suffer from the scalability problems on large clusters of thousands of cores.  
+To enhance the robustness of Krylov iterative solvers, some techniques have been proposed allowing the use of different preconditioners, if necessary, within the iteration instead of restarting. Those techniques may lead to considerable savings in CPU time and memory requirements. Van der Vorst in~\cite{Vorst94} has for instance proposed variants of the GMRES algorithm in which a different preconditioner is applied in each iteration, leading to the so-called GMRESR family of nested methods. In fact, the GMRES method is effectively preconditioned with other iterative schemes (or GMRES itself), where the iterations of the GMRES method are called outer iterations while the iterations of the preconditioning process is referred to as inner iterations. Saad in~\cite{Saad:1993} has proposed FGMRES which is another variant of the GMRES algorithm using a variable preconditioner. In FGMRES the search directions are preconditioned whereas in GMRESR the residuals are preconditioned. However, in practice, good preconditioners are those based on direct methods, as ILU preconditioners, which are not easy to parallelize and suffer from the scalability problems on large clusters of thousands of cores.  
 
 Recently, communication-avoiding methods have been developed to reduce the communication overheads in Krylov subspace iterative solvers. On modern computer architectures, communications between processors are much slower than floating-point arithmetic operations on a given processor. Communication-avoiding techniques reduce either communications between processors or data movements between levels of the memory hierarchy, by reformulating the communication-bound kernels (more frequently SpMV kernels) and the orthogonalization operations within the Krylov iterative solver. Different works have studied the communication-avoiding techniques for the GMRES method, so-called CA-GMRES, on multicore processors and multi-GPU machines~\cite{Mohiyuddin2009,Hoemmen2010,Yamazaki2014}. 
 
@@ -705,7 +705,7 @@ method. Moreover,  a tolerance  threshold must be  specified for the  solver. In
 practice, this threshold must be  much smaller than the convergence threshold of
 the TSIRM  algorithm (\emph{i.e.},  $\epsilon_{tsirm}$).  We also  consider that
 after  the call of  the $Solve$  function, we  obtain the  vector $x_k$  and the
-$error$ which is defined by $||Ax_k-b||_2$.
+$error$, which is defined by $||Ax_k-b||_2$.
 
   Line~\ref{algo:store},  $S_{k \mod  s}=x_k$ consists  in copying  the solution
   $x_k$ into the  column $k \mod s$ of $S$.  After  the minimization, the matrix
@@ -716,7 +716,7 @@ $error$ which is defined by $||Ax_k-b||_2$.
 
 Let us summarize the most important parameters of TSIRM:
 \begin{itemize}
-\item $\epsilon_{tsirm}$: the threshold to stop the TSIRM method;
+\item $\epsilon_{tsirm}$: the threshold that stops the TSIRM method;
 \item $max\_iter_{kryl}$: the maximum number of iterations for the Krylov method;
 \item $s$: the number of outer iterations before applying the minimization step;
 \item $max\_iter_{ls}$: the maximum number of iterations for the iterative least-squares method;
@@ -727,9 +727,9 @@ Let us summarize the most important parameters of TSIRM:
 The  parallelization  of  TSIRM  relies   on  the  parallelization  of  all  its
 parts. More  precisely, except  the least-squares step,  all the other  parts are
 obvious to  achieve out in parallel. In  order to develop a  parallel version of
-our   code,   we   have   chosen  to   use   PETSc~\cite{petsc-web-page}.    For
-line~\ref{algo:matrix_mul} the  matrix-matrix multiplication is  implemented and
-efficient since the  matrix $A$ is sparse and since the  matrix $S$ contains few
+our   code,   we   have   chosen  to   use   PETSc~\cite{petsc-web-page}.    In
+line~\ref{algo:matrix_mul}, the  matrix-matrix multiplication is  implemented and
+efficient since the  matrix $A$ is sparse and the  matrix $S$ contains few
 columns in  practice. As explained  previously, at least  two methods seem  to be
 interesting to solve the least-squares minimization, CGLS and LSQR.
 
@@ -764,7 +764,7 @@ the parallelization of CGLS which is  similar to LSQR.
 
 
 In each iteration  of CGLS, there is two  matrix-vector multiplications and some
-classical  operations:  dot  product,   norm,  multiplication  and  addition  on
+classical  operations:  dot  product,   norm,  multiplication,  and  addition  on
 vectors.  All  these  operations are  easy  to  implement  in PETSc  or  similar
 environment.  It should be noticed that LSQR follows the same principle, it is a
 little bit longer but it performs more or less the same operations.
@@ -846,8 +846,11 @@ $\begin{array}{ll}
 which concludes the induction and the proof.
 \end{proof}
 
-%We can remark that, at each iterate, the residue of the TSIRM algorithm is lower 
-%than the one of the GMRES method.
+Remark that a similar proposition can be formulated at each time
+the given solver satisfies an inequality of the form $||r_n|| \leqslant \mu^n ||r_0||$,
+with $|\mu|<1$. Furthermore, it is \emph{a priori} possible in some particular cases 
+regarding $A$, 
+that the proposed TSIRM converges while the GMRES($m$) does not.
 
 %%%*********************************************************
 %%%*********************************************************
@@ -881,13 +884,14 @@ torso3             & 2D/3D problem & 259,156 & 4,429,042 \\
 \label{tab:01}
 \end{center}
 \end{table}
-Chosen parameters  are detailed below.   As by default  the restart of  GMRES is
-performed  every 30  iterations,  we have  chosen  to stop  the  GMRES every  30
-iterations (\emph{i.e.} $max\_iter_{kryl}=30$).  $s$ is set to 8. CGLS is chosen
-to   minimize  the   least-squares  problem   with  the   following  parameters:
+Chosen parameters  are detailed below.   
+We have  stopped  the  GMRES every  30
+iterations (\emph{i.e.}, $max\_iter_{kryl}=30$), which is the default 
+setting of GMRES.  $s$, for its part, has been set to 8. CGLS 
+ minimizes  the   least-squares  problem   with  parameters
 $\epsilon_{ls}=1e-40$ and $max\_iter_{ls}=20$.  The external precision is set to
-$\epsilon_{tsirm}=1e-10$.  Those  experiments have been performed  on a Intel(R)
-Core(TM) i7-3630QM CPU @ 2.40GHz with the version 3.5.1 of PETSc.
+$\epsilon_{tsirm}=1e-10$.  These  experiments have been performed  on an Intel(R)
+Core(TM) i7-3630QM CPU @ 2.40GHz with the 3.5.1 version  of PETSc.
 
 
 In  Table~\ref{tab:02}, some  experiments comparing  the solving  of  the linear
@@ -1174,11 +1178,13 @@ experiments up to 16,394 cores have been led to verify that TSIRM runs
 
 
 For  future  work, the  authors'  intention is  to  investigate  other kinds  of
-matrices, problems, and  inner solvers. The influence of  all parameters must be
+matrices, problems, and  inner solvers. In particular, the possibility 
+to obtain a convergence of TSIRM in situations where the GMRES is divergent will be
+investigated. The influence of  all parameters must be
 tested too, while other methods to minimize the residuals must be regarded.  The
 number of outer  iterations to minimize should become  adaptative to improve the
 overall performances of the proposal.   Finally, this solver will be implemented
-inside PETSc. This  would be very interesting because it would  allow us to test
+inside PETSc, which would be of interest as it would  allow us to test
 all the non-linear  examples and compare our algorithm  with the other algorithm
 implemented in PETSc.
 
