X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/GMRES2stage.git/blobdiff_plain/2fc464daa5a04774f5fa10bd96d36c53cc908a4a..3aa4a4a5934c50b8ee7ac223ae1ebc31796c820c:/paper.tex

diff --git a/paper.tex b/paper.tex
index 54e35d3..2372b61 100644
--- a/paper.tex
+++ b/paper.tex
@@ -754,7 +754,7 @@ In order to see the influence of our algorithm with only one processor, we first
 show  a comparison  with the  standard version  of GMRES  and our  algorithm. In
 Table~\ref{tab:01},  we  show  the  matrices  we  have used  and  some  of  them
 characteristics. For all  the matrices, the name, the field,  the number of rows
-and the number of nonzero elements is given.
+and the number of nonzero elements are given.
 
 \begin{table}[htbp]
 \begin{center}
@@ -777,7 +777,7 @@ torso3             & 2D/3D problem & 259,156 & 4,429,042 \\
 
 The following  parameters have been chosen  for our experiments.   As by default
 the restart  of GMRES is performed every  30 iterations, we have  chosen to stop
-the GMRES every 30 iterations, $max\_iter_{kryl}=30$).  $s$ is set to 8. CGLS is
+the GMRES every 30 iterations (\emph{i.e.} $max\_iter_{kryl}=30$).  $s$ is set to 8. CGLS is
 chosen  to minimize  the least-squares  problem with  the  following parameters:
 $\epsilon_{ls}=1e-40$ and $max\_iter_{ls}=20$.  The external precision is set to
 $\epsilon_{tsirm}=1e-10$.  Those  experiments have been performed  on a Intel(R)
@@ -789,7 +789,7 @@ systems obtained with the previous matrices  with a GMRES variant and with out 2
 stage algorithm are  given. In the second column, it can  be noticed that either
 gmres or fgmres is used to  solve the linear system.  According to the matrices,
 different  preconditioner is used.   With TSIRM,  the same  solver and  the same
-preconditionner is used.  This Table shows that TSIRM can drastically reduce the
+preconditionner are used.  This Table shows that TSIRM can drastically reduce the
 number of iterations to reach the  convergence when the number of iterations for
 the normal GMRES is more or less  greater than 500. In fact this also depends on
 tow  parameters: the  number  of iterations  to  stop GMRES  and  the number  of
@@ -823,12 +823,12 @@ torso3             & fgmres / sor  & 37.70 & 565 & 34.97 & 510 \\
 
 
 
-In order to perform larger  experiments, we have tested some example application
+In order to perform larger  experiments, we have tested some example applications
 of PETSc. Those  applications are available in the ksp part  which is suited for
 scalable linear equations solvers:
 \begin{itemize}
 \item ex15  is an example  which solves in  parallel an operator using  a finite
-  difference  scheme.   The  diagonal  is  equals to  4  and  4  extra-diagonals
+  difference  scheme.   The  diagonal  is  equal to  4  and  4  extra-diagonals
   representing the neighbors in each directions  is equal to -1. This example is
   used  in many  physical phenomena, for  example, heat  and fluid  flow, wave
   propagation...
@@ -940,7 +940,7 @@ the number of iterations. So, the overall benefit of using TSIRM is interesting.
 \end{table*}
 
 
-In Table~\ref{tab:04}, some experiments with example ex54 on the Curie architecture are reported
+In Table~\ref{tab:04}, some experiments with example ex54 on the Curie architecture are reported.
 
 
 \begin{table*}[htbp]
