X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/GMRES2stage.git/blobdiff_plain/7122f8d886bcd6191b7eee5017e8c96944ab7e56..ea8220acf828703b413185d8e722719b6664614f:/IJHPCN/paper.tex

diff --git a/IJHPCN/paper.tex b/IJHPCN/paper.tex
index db5f791..2d0bd55 100644
--- a/IJHPCN/paper.tex
+++ b/IJHPCN/paper.tex
@@ -1035,80 +1035,23 @@ cores to more than 16 with 8,192 cores.
 \subsection{Influence of parameters for TSIRM}
 In this section we present some experimental results in order to study the influence of some parameters on the TSIRM algorithm. We conducted experiments on $16$ cores to solve 3D problems of size $200,000$ components per core. We solved nonlinear problems token from examples of PETSc. We fixed some parameters of the TSIRM algorithm as follows: the nonlinear systems are solved with a precision of $10^{-8}$, block Jacobi preconditioner is used, the tolerance threshold $\epsilon_{tsirm}$ is $10^{-8}$ , the maximum number of iterations $max\_iter_{tsirm}$ is set to $10,000$ iterations, the FGMRES method is used as the inner solver with a tolerance threshold $\epsilon_{kryl}=10^{-10}$ and the least-squares problem is solved with a precision $\epsilon_{ls}=10^{-40}$ in the minimization process.
 
-%time mpirun ../ex48 -da_grid_x 147 -da_grid_y 147 -da_grid_z 147 -snes_rtol 1.e-8 -snes_monitor -ksp_type tsirm -ksp_pc_type bjacobi -pc_type ksp -ksp_tsirm_tol 1e-8 -ksp_tsirm_maxiter 10000 -ksp_ksp_type fgmres -ksp_tsirm_max_inner_iter 30 -ksp_tsirm_inner_restarts 30 -ksp_tsirm_inner_tol 1e-10 -ksp_tsirm_cgls 0 -ksp_tsirm_tol_ls 1.e-40 -ksp_tsirm_maxiter_ls 15 -ksp_tsirm_size_ls 10 
+%time mpirun ../ex34 -da_grid_x 147 -da_grid_y 147 -da_grid_z 147 -ksp_type tsirm -ksp_pc_type asm -pc_type ksp -ksp_tsirm_tol 1e-10 -ksp_tsirm_maxiter 10000 -ksp_ksp_type fgmres -ksp_tsirm_max_inner_iter 30 -ksp_tsirm_inner_tol 1e-10 -ksp_tsirm_cgls 0 -ksp_tsirm_tol_ls 1.e-40 -ksp_tsirm_maxiter_ls 20 -ksp_tsirm_size_ls 10
 \begin{figure}[htbp]
 \centering
-  \includegraphics[angle=-90,width=0.5\textwidth]{ksp_tsirm_cgls_iter_total}
-\caption{Number of total iterations using two different methods for the minimization: LSQR and CGLS.}
-\label{fig:cgls-iter} 
+  \includegraphics[width=0.5\textwidth]{ksp_tsirm_cgls}
+\caption{Number of total iterations using two different methods for the minimization: CGLS and LSQR.}
+\label{fig:cgls} 
 \end{figure}
 
 \begin{figure}[htbp]
 \centering
-  \includegraphics[angle=-90,width=0.5\textwidth]{ksp_tsirm_cgls_time}
-\caption{Execution time in seconds using two different methods for the minimization: LSQR and CGLS.}
-\label{fig:cgls-time} 
+  \includegraphics[width=0.5\textwidth]{snes_ex14}
+\caption{Total number of iterations in example {\it snes ex14} of PETSc by varyin the number of inner iterations and the size of the least-squares problem.}
+\label{fig:snes_ex14} 
 \end{figure}
 
-%time mpirun ../ex35 -da_grid_x 147 -da_grid_y 147 -da_grid_z 147 -snes_rtol 1.e-8 -snes_monitor -ksp_type tsirm -ksp_pc_type bjacobi -pc_type ksp -ksp_tsirm_tol 1e-8 -ksp_tsirm_maxiter 10000 -ksp_ksp_type fgmres -ksp_tsirm_max_inner_iter 30 -ksp_tsirm_inner_restarts 38 -ksp_tsirm_inner_tol 1e-10 -ksp_tsirm_cgls 0 -ksp_tsirm_tol_ls 1.e-40 -ksp_tsirm_maxiter_ls 15 -ksp_tsirm_size_ls 10
-\begin{figure}[htbp]
-\centering
-  \includegraphics[angle=-90,width=0.5\textwidth]{ksp_tsirm_inner_restarts_iter_total}
-\caption{Number of total iterations with variation of restarts in the inner solver FGMRES.}
-\label{fig:inner_restarts_iter_total} 
-\end{figure}
 
-\begin{figure}[htbp]
-\centering
-  \includegraphics[angle=-90,width=0.5\textwidth]{ksp_tsirm_inner_restarts_time}
-\caption{Execution time in seconds with variation of restarts in the inner solver FGMRES.}
-\label{fig:inner_restarts_time} 
-\end{figure}
 
-%time mpirun ../ex14 -da_grid_x 147 -da_grid_y 147 -da_grid_z 147 -snes_rtol 1.e-8 -snes_monitor -ksp_type tsirm -ksp_pc_type bjacobi -pc_type ksp -ksp_tsirm_tol 1e-8 -ksp_tsirm_maxiter 10000 -ksp_ksp_type fgmres -ksp_tsirm_max_inner_iter 1000 -ksp_tsirm_inner_restarts 30 -ksp_tsirm_inner_tol 1e-10 -ksp_tsirm_cgls 0 -ksp_tsirm_tol_ls 1.e-40 -ksp_tsirm_maxiter_ls 15 -ksp_tsirm_size_ls 10
-\begin{figure}[htbp]
-\centering
-  \includegraphics[angle=-90,width=0.5\textwidth]{ksp_tsirm_max_inner_iter}
-\caption{Number of total iterations with variation of number of inner iterations.}
-\label{fig:max_inner_iter} 
-\end{figure}
-
-\begin{figure}[htbp]
-\centering
-  \includegraphics[angle=-90,width=0.5\textwidth]{ksp_tsirm_max_inner_time}
-\caption{Execution time in seconds with variation of number of inner iterations.}
-\label{fig:max_inner_time} 
-\end{figure}
-
-%time mpirun ../ex14 -da_grid_x 147 -da_grid_y 147 -da_grid_z 147 -snes_rtol 1.e-8 -snes_monitor -ksp_type tsirm -ksp_pc_type bjacobi -pc_type ksp -ksp_tsirm_tol 1e-8 -ksp_tsirm_maxiter 10000 -ksp_ksp_type fgmres -ksp_tsirm_max_inner_iter 30 -ksp_tsirm_inner_restarts 30 -ksp_tsirm_inner_tol 1e-10 -ksp_tsirm_cgls 0 -ksp_tsirm_tol_ls 1.e-40 -ksp_tsirm_maxiter_ls 5 -ksp_tsirm_size_ls 10
-\begin{figure}[htbp]
-\centering
-  \includegraphics[angle=-90,width=0.5\textwidth]{ksp_tsirm_maxiter_ls_iter}
-\caption{Number of total iterations with variation of number of iterations in the minimization process.}
-\label{fig:maxiter_ls_iter} 
-\end{figure}
-
-\begin{figure}[htbp]
-\centering
-  \includegraphics[angle=-90,width=0.5\textwidth]{ksp_tsirm_maxiter_ls_time}
-\caption{Execution time in seconds with variation of number of iterations in the minimization process.}
-\label{fig:maxiter_ls_time} 
-\end{figure}
-
-%time mpirun ../ex14 -da_grid_x 147 -da_grid_y 147 -da_grid_z 147 -snes_rtol 1.e-8 -snes_monitor -ksp_type tsirm -ksp_pc_type bjacobi -pc_type ksp -ksp_tsirm_tol 1e-8 -ksp_tsirm_maxiter 10000 -ksp_ksp_type fgmres -ksp_tsirm_max_inner_iter 30 -ksp_tsirm_inner_restarts 30 -ksp_tsirm_inner_tol 1e-10 -ksp_tsirm_cgls 0 -ksp_tsirm_tol_ls 1.e-40 -ksp_tsirm_maxiter_ls 15 -ksp_tsirm_size_ls 2
-\begin{figure}[htbp]
-\centering
-  \includegraphics[angle=-90,width=0.5\textwidth]{ksp_tsirm_size_ls_iter}
-\caption{Number of total iterations with variation of the size of the least-squares problem in the minimization process.}
-\label{fig:size_ls_iter} 
-\end{figure}
-
-\begin{figure}[htbp]
-\centering
-  \includegraphics[angle=-90,width=0.5\textwidth]{ksp_tsirm_size_ls_time}
-\caption{Execution time in seconds with variation of the size of the least-squares problem in the minimization process.}
-\label{fig:size_ls_time} 
-\end{figure}
 
 %%ENDNEW
 
