X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/GMRES2stage.git/blobdiff_plain/eacf4c2eeca7315f0a4a7bc9dec99dc6778843d1..649421a46874291325940af659c9eb66d83411b4:/paper.tex

diff --git a/paper.tex b/paper.tex
index 4d59b93..f4dba97 100644
--- a/paper.tex
+++ b/paper.tex
@@ -1035,8 +1035,40 @@ the number of iterations. So, the overall benefit of using TSIRM is interesting.
 \end{table*}
 
 
-In Table~\ref{tab:04}, some experiments with example ex54 on the Curie architecture are reported.
-
+In  Table~\ref{tab:04},  some  experiments   with  example  ex54  on  the  Curie
+architecture are reported.  For this  application, we fixed $\alpha=0.6$.  As it
+can be seen in that Table, the size of the problem has a strong influence on the
+number of iterations to reach the  convergence. That is why we have preferred to
+change the threshold.  If we set  it to $1e-3$ as with the previous application,
+only one iteration is necessray  to reach the convergence. So Table~\ref{tab:04}
+shows the results  of differents executions with differents  number of cores and
+differents thresholds. As  with the previous example, we  can observe that TSIRM
+is faster than FGMRES. The ratio greatly depends on the number of iterations for
+FMGRES to reach the threshold. The greater the number of iterations to reach the
+convergence is, the  better the ratio between our algorithm  and FMGRES is. This
+experiment is  also a  weak scaling with  approximately $25,000$  components per
+core. It can also  be observed that the difference between CGLS  and LSQR is not
+significant. Both can be good but it seems not possible to know in advance which
+one will be the best.
+
+Table~\ref{tab:05} show a strong scaling experiment with the exemple ex54 on the
+Curie  architecture. So  in  this case,  the  number of  unknownws  is fixed  to
+$204,919,225$ and the number of cores ranges from $512$ to $8192$ with the power
+of two.  The  threshold is fixed to $5e-5$ and only  the $mg$ preconditioner has
+been tested. Here  again we can see that TSIRM is  faster that FGMRES. Efficiecy
+of each algorithms is reported. It  can be noticed that FGMRES is more efficient
+than TSIRM except with $8,192$ cores and that its efficiency is greater that one
+whereas the  efficiency of TSIRM is  lower than one. Nevertheless,  the ratio of
+TSIRM  with any  version  of the  least-squares  method is  always faster.  With
+$8,192$ cores when the number of iterations is far more important for FGMRES, we
+can see that it is only slightly more important for TSIRM.
+
+In  Figure~\ref{fig:02}  we report  the  number  of  iterations per  second  for
+experiments  reported in  Table~\ref{tab:05}.  This Figure  highlights that  the
+number of iterations per  seconds is more of less the same  for FGMRES and TSIRM
+with a little advantage for FGMRES. It  can be explained by the fact that, as we
+have previously explained, that the iterations of the least-sqaure steps are not
+taken into account with TSIRM.
 
 \begin{table*}[htbp]
 \begin{center}
