X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/JournalMultiPeriods.git/blobdiff_plain/c882850ec6da71a9df727591d68e24b4319c7fdd..417b105e08f70d1019f3df8e026fb2c76da601c2:/reponse.tex?ds=inline

diff --git a/reponse.tex b/reponse.tex
index 654a1d1..0edaada 100644
--- a/reponse.tex
+++ b/reponse.tex
@@ -120,7 +120,7 @@ Computing the average energy consumption per unit of time over the network
 lifetime would be better, as it is independent from the number and duration of
 rounds.  \\
 
-\textcolor{blue}{\textbf{\textsc{Answer :}        }}
+\textcolor{blue}{\textbf{\textsc{Answer :} Yes, you  are  right. It is possible to obtain the average energy consumption per unit of time by dividing the criterion defined in section .... by the round duration.}}
 
 
 
