X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/Sensornets15.git/blobdiff_plain/f6ed458a211eb088e2e1f4e18f77423682ea034f..HEAD:/ahswn.tex?ds=inline

diff --git a/ahswn.tex b/ahswn.tex
index e2ef23c..d66df5d 100644
--- a/ahswn.tex
+++ b/ahswn.tex
@@ -18,7 +18,7 @@
 
 \institute{FEMTO-ST Institute, UMR 6174 CNRS, University of Franche-Comt\'e, France}
 
-\def\received{Received 21 October 2014}
+\def\received{Received 23 October 2014}
 
 \maketitle
 
@@ -437,19 +437,20 @@ experimental results  which are relevant. The  nodes are deployed on  a field of
 interest of $(50 \times 25)~m^2 $ in such a way that they cover the field with a
 high coverage ratio.
 
-We  chose as  energy  consumption  model the  one  proposed proposed  \linebreak
-by~\cite{ChinhVu}  and   based  on  ~\cite{raghunathan2002energy}   with  slight
-modifications. The energy  consumed by the communications is  added and the part
-relative to a  variable sensing range is removed. We also  assume that the nodes
-have   the   characteristics   of   the   Medusa   II   sensor   node   platform
-\cite{raghunathan2002energy}.  A sensor node typically consists of four units: a
-MicroController Unit, an Atmels AVR ATmega103L  in case of Medusa II, to perform
-the  computations;  a  communication  (radio)  unit able  to  send  and  receive
-messages; a  sensing unit  to collect  data; a power  supply which  provides the
-energy consumed by node. Except the  battery, all the other unit can be switched
-off to save energy according  to the node status.  Table~\ref{table4} summarizes
-the energy consumed (in milliWatt per second) by a node for each of its possible
-status.
+We   chose   as   energy    consumption   model   the   one   proposed
+by~\cite{ChinhVu}  and  based  on  ~\cite{raghunathan2002energy}  with
+slight  modifications. The  energy consumed  by the  communications is
+added and the part relative to a variable sensing range is removed. We
+also assume that  the nodes have the characteristics  of the Medusa II
+sensor  node  platform  \cite{raghunathan2002energy}.  A  sensor  node
+typically consists  of four units:  a MicroController Unit,  an Atmels
+AVR ATmega103L  in case of Medusa  II, to perform  the computations; a
+communication  (radio)  unit able  to  send  and  receive messages;  a
+sensing unit to collect data; a power supply which provides the energy
+consumed  by node.  Except  the battery,  all  the other  unit can  be
+switched   off  to  save   energy  according   to  the   node  status.
+Table~\ref{table4}  summarizes the energy  consumed (in  milliWatt per
+second) by a node for each of its possible status.
 
 \begin{table}
 \caption{Energy consumption model.}
@@ -527,7 +528,7 @@ the efficiency of our approach:
   where  $n$ is  the number  of covered  grid points  by active  sensors  of every
   subregions during  the current  sensing phase  and $N$ is the total number  of grid
   points in  the sensing field. In  our simulations, we have  a layout of  $N = 51
-  \times 26 = 1326$ grid points.
+  \times 26 = 1,326$ grid points.
 
 \item {{\bf  Energy Consumption}:}  energy consumption (EC)  can be seen  as the
   total amount of  energy   consumed   by   the   sensors   during   $Lifetime_{95}$   
@@ -591,7 +592,7 @@ nodes, and thus enables the extension of the lifetime.
 \begin{center}
 \scalebox{0.5}{\includegraphics{R/CR.pdf}}
 \end{center}
-\caption{Coverage ratio}
+\caption{Coverage ratio.}
 \label{fig3}
 \end{figure} 
 
