X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/025698f711cfa8d174abdf309b09da921696771e..refs/heads/master:/CHAPITRE_04.tex?ds=sidebyside

diff --git a/CHAPITRE_04.tex b/CHAPITRE_04.tex
index ff3f8f7..b518209 100644
--- a/CHAPITRE_04.tex
+++ b/CHAPITRE_04.tex
@@ -20,7 +20,7 @@ divided  into subregions using  a divide-and-conquer  algorithm and  an activity
 
 The remainder of this chapter is organized as follows. The next section is devoted to the DiLCO protocol description. Section \ref{ch4:sec:03} gives the primary points based coverage problem formulation which is used to schedule the activation of sensors. Section \ref{ch4:sec:04} shows the simulation results obtained using the discrete event simulator OMNeT++ \cite{ref158}. They fully demonstrate the usefulness of the proposed approach. Finally, we give concluding remarks in section \ref{ch4:sec:05}.
 
-
+\vfill
 
 \section{Description of the DiLCO Protocol}
 \label{ch4:sec:02}
@@ -191,7 +191,7 @@ Active  sensors  in the  period  will  execute  their sensing  task  to preserve
 
 An outline of the  protocol implementation is given by Algorithm~\ref{alg:DiLCO} which describes the execution of a period  by a node (denoted by $s_j$  for a sensor  node indexed by  $j$). In  the beginning,  a node  checks whether  it has enough energy to stay active during the next sensing phase (i.e., the remaining energy $RE_j$ $\geq$ $E_{th}$ (the  amount of energy required to be alive during one period)). If yes, it exchanges information  with  all the  other nodes belonging to the same subregion:  it collects from each node its position coordinates, remaining energy ($RE_j$), ID, and  the number  of  one-hop neighbors  still  alive. Once  the  first phase  is completed, the nodes  of a subregion choose a leader to  take the decision based on the criteria described in section \ref{ch4:sec:02:03:02}.
 %the  following  criteria   with  decreasing  importance:  larger  number  of neighbors, larger remaining energy, and  then in case of equality, larger index. 
-After that,  if the sensor node is  leader, it will execute  the integer program algorithm (see Section~\ref{ch4:sec:03})  which provides a set of  sensors planned to be active in the next sensing phase. As leader, it will send an ActiveSleep packet to each sensor  in the same subregion to  indicate it if it has to  be active or not.  Alternately, if  the  sensor  is not  the  leader, it  will  wait for  the ActiveSleep packet to know its state for the coming sensing phase. \textcolor{blue}{The flowchart of DiLCO protocol executed in each sensor node is presented in Figure \ref{flow4}.} 
+After that,  if the sensor node is  leader, it will execute  the integer program algorithm (see Section~\ref{ch4:sec:03})  which provides a set of  sensors planned to be active in the next sensing phase. As leader, it will send an ActiveSleep packet to each sensor  in the same subregion to  indicate it if it has to  be active or not.  Alternately, if  the  sensor  is not  the  leader, it  will  wait for  the ActiveSleep packet to know its state for the coming sensing phase. The flowchart of DiLCO protocol executed in each sensor node is presented in Figure \ref{flow4}. 
 
 \begin{figure}[ht!]
 \centering
@@ -747,27 +747,37 @@ In fact,  the distribution of computation over the subregions greatly reduces th
 As highlighted by Figures~\ref{Figures/ch4/R3/LT}(a) and \ref{Figures/ch4/R3/LT}(b), the network lifetime obviously increases when the size of the network increases, with DiLCO-16 protocol and DiLCO-32 protocol which lead to maximize the lifetime of the network compared with other approaches. 
 %In figures~\ref{Figures/ch4/R3/LT95} and \ref{Figures/ch4/R3/LT50}, network lifetime, $Lifetime95$ and $Lifetime50$ respectively, are illustrated for different network sizes.  
 
-\begin{figure}[h!]
-\centering
+%%\begin{figure}[p!]
+%%\centering
 % \begin{multicols}{0}
-\centering
-\includegraphics[scale=0.8]{Figures/ch4/R3/LT95.eps}\\~ ~ ~ ~ ~(a) \\
+%%\centering
+%%\includegraphics[scale=0.8]{Figures/ch4/R3/LT95.eps}\\~ ~ ~ ~ ~(a) \\
 %\hfill 
-\includegraphics[scale=0.8]{Figures/ch4/R3/LT50.eps}\\~ ~ ~ ~ ~(b)
+%%\includegraphics[scale=0.8]{Figures/ch4/R3/LT50.eps}\\~ ~ ~ ~ ~(b)
 
 %\end{multicols} 
-\caption{Network lifetime for (a) $Lifetime_{95}$ and (b) $Lifetime_{50}$}
-  \label{Figures/ch4/R3/LT}
-\end{figure}
+%%\caption{Network lifetime for (a) $Lifetime_{95}$ and (b) $Lifetime_{50}$}
+%%  \label{Figures/ch4/R3/LT}
+%%\end{figure}
 
 
 By choosing the best suited nodes, for each period, by optimizing the coverage and lifetime of the network to cover the area of interest and by letting the other ones sleep in order to be used later in next periods, DiLCO-16 protocol and DiLCO-32 protocol efficiently prolong the network lifetime. 
 Comparison shows that DiLCO-16 protocol and DiLCO-32 protocol, which use distributed optimization over the subregions, are the best ones because they are robust to network disconnection during the network lifetime as well as they consume less energy in comparison with other approaches. 
 %It also means that distributing the algorithm in each node and subdividing the sensing field into many subregions, which are managed independently and simultaneously, is the most relevant way to maximize the lifetime of a network.
 
-
 \end{enumerate}
+\begin{figure}[p!]
+\centering
+% \begin{multicols}{0}
+\centering
+\includegraphics[scale=0.8]{Figures/ch4/R3/LT95.eps}\\~ ~ ~ ~ ~(a) \\
+%\hfill 
+\includegraphics[scale=0.8]{Figures/ch4/R3/LT50.eps}\\~ ~ ~ ~ ~(b)
 
+%\end{multicols} 
+\caption{Network lifetime for (a) $Lifetime_{95}$ and (b) $Lifetime_{50}$}
+  \label{Figures/ch4/R3/LT}
+\end{figure}
 \section{Conclusion}
 \label{ch4:sec:05}
 A crucial problem in WSN is to schedule the sensing activities of the different nodes  in order to ensure both coverage of  the area  of interest  and longer network lifetime. The inherent limitations of sensor nodes, in energy provision, communication, and computing capacities,  require protocols that optimize the use of the  available resources  to  fulfill the sensing  task. To address  this problem, this chapter proposes a  two-step approach. Firstly, the field of sensing
