X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/0a4831505b7eaf36f78bc512ac5c62f033fe0d59..5b873620b230517c1592c89c4c8dd5dba2818339:/CHAPITRE_04.tex?ds=sidebyside

diff --git a/CHAPITRE_04.tex b/CHAPITRE_04.tex
index edbf259..c359b8b 100644
--- a/CHAPITRE_04.tex
+++ b/CHAPITRE_04.tex
@@ -342,7 +342,7 @@ The modeling language for Mathematical Programming (AMPL)~\cite{AMPL} is  employ
 
 \indent In this dissertation, we used an energy consumption model proposed by~\cite{DESK} and based on \cite{ref112} with slight  modifications.  The energy consumption for  sending/receiving the packets is added, whereas the  part related to the dynamic sensing range is removed because we consider a fixed sensing range.
 
-\indent For our energy consumption model, we refer to the sensor node Medusa~II which uses an Atmel's  AVR ATmega103L microcontroller~\cite{ref112}. The typical architecture  of a  sensor  is composed  of four  subsystems: the  MCU subsystem which is capable of computation, communication subsystem (radio) which is responsible  for transmitting/receiving messages, the  sensing subsystem that collects  data, and  the  power supply  which  powers the  complete sensor  node \cite{ref112}. Each  of the first three subsystems  can be turned on or  off depending on  the current status  of the sensor.   Energy consumption (expressed in  milliWatt per second) for  the different status of  the sensor is summarized in Table~\ref{table1}.
+\indent For our energy consumption model, we refer to the sensor node Medusa~II which uses an Atmel's  AVR ATmega103L microcontroller~\cite{ref112}. The typical architecture  of a  sensor  is composed  of four  subsystems: the  MCU subsystem which is capable of computation, communication subsystem (radio) which is responsible  for transmitting/receiving messages, the  sensing subsystem that collects  data, and  the  power supply  which  powers the  complete sensor  node \cite{ref112}. Each  of the first three subsystems  can be turned on or  off depending on  the current status  of the sensor.   Energy consumption (expressed in  milliWatt per second) for  the different status of  the sensor is summarized in Table~\ref{tab:EC}.
 
 \begin{table}[h]
 \centering
