X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/0a4831505b7eaf36f78bc512ac5c62f033fe0d59..cd18d10c8b21709c65c71c19c28340bb9d82a5bc:/CHAPITRE_05.tex

diff --git a/CHAPITRE_05.tex b/CHAPITRE_05.tex
index 733232c..6604d95 100644
--- a/CHAPITRE_05.tex
+++ b/CHAPITRE_05.tex
@@ -41,11 +41,6 @@ mechanisms: subdividing the area of interest into several subregions (like a clu
 
 As can be seen in Figure~\ref{fig2},  our protocol  works in  periods fashion, where  each is  divided  into 4  phases: Information~Exchange,  Leader~Election, Decision, and Sensing. 
 %The information exchange among wireless sensor nodes is described in chapter 4, section \ref{ch4:sec:02:03:01}. The leader election in each subregion is explained in chapter 4, section \ref{ch4:sec:02:03:02}, 
-The difference with MuDiLCO in that the elected leader in each subregion is for each period. In the decision phase, each leader will solve an integer  program to select which  cover sets  will be activated in  the following  sensing phase  to cover the  subregion to  which it belongs.  The integer  program will produce $T$ cover sets,  one for each round. The leader will send an ActiveSleep  packet to each sensor in the subregion based on the algorithm's results, indicating if the sensor should be active or not in
-each round  of the  sensing phase. Each sensing phase is itself divided into $T$ rounds and for each round a set of sensors (a cover set) is responsible for the sensing task. 
-%Each sensor node in the subregion will receive an ActiveSleep packet from leader, informing it to stay awake or to go to sleep for  each round of the sensing  phase. 
-Algorithm~\ref{alg:MuDiLCO}, which will be  executed by each node at the beginning  of a period, explains  how the ActiveSleep packet is obtained. In this way, a multiround optimization  process is performed  during each
-period  after  Information~Exchange  and  Leader~Election phases,  in  order to produce $T$ cover sets that will take the mission of sensing for $T$ rounds.
 \begin{figure}[ht!]
 \centering \includegraphics[width=160mm]{Figures/ch5/GeneralModel.jpg} % 70mm  Modelgeneral.pdf
 \caption{MuDiLCO protocol.}
@@ -53,12 +48,6 @@ period  after  Information~Exchange  and  Leader~Election phases,  in  order to
 \end{figure} 
 
 
-%This protocol minimizes the impact of unexpected node failure (not due to batteries running out of energy), because it works in periods. On the one hand, if a node failure is detected before making the decision, the node will not participate during this phase. On the other hand, if the node failure occurs after the decision, the sensing  task of the network will be temporarily affected:  only during  the period of sensing until a new period starts.
-
-%The  energy consumption  and some other constraints  can easily  be  taken into account since the  sensors  can  update and  then  exchange their  information (including their residual energy) at the beginning of each period.  However, the pre-sensing  phases (Information  Exchange, Leader  Election, and  Decision) are energy  consuming for some  nodes, even  when they  do not  join the  network to monitor the area.
-
- 
-
 \begin{algorithm}[h!]                
  % \KwIn{all the parameters related to information exchange}
 %  \KwOut{$winer-node$ (: the id of the winner sensor node, which is the leader of current round)}
@@ -99,6 +88,19 @@ period  after  Information~Exchange  and  Leader~Election phases,  in  order to
 
 \end{algorithm}
 
+The difference with MuDiLCO in that the elected leader in each subregion is for each period. In the decision phase, each leader will solve an integer  program to select which  cover sets  will be activated in  the following  sensing phase  to cover the  subregion to  which it belongs.  The integer  program will produce $T$ cover sets,  one for each round. The leader will send an ActiveSleep  packet to each sensor in the subregion based on the algorithm's results, indicating if the sensor should be active or not in
+each round  of the  sensing phase. Each sensing phase is itself divided into $T$ rounds and for each round a set of sensors (a cover set) is responsible for the sensing task. 
+%Each sensor node in the subregion will receive an ActiveSleep packet from leader, informing it to stay awake or to go to sleep for  each round of the sensing  phase. 
+Algorithm~\ref{alg:MuDiLCO}, which will be  executed by each node at the beginning  of a period, explains  how the ActiveSleep packet is obtained. In this way, a multiround optimization  process is performed  during each
+period  after  Information~Exchange  and  Leader~Election phases,  in  order to produce $T$ cover sets that will take the mission of sensing for $T$ rounds.
+
+
+%This protocol minimizes the impact of unexpected node failure (not due to batteries running out of energy), because it works in periods. On the one hand, if a node failure is detected before making the decision, the node will not participate during this phase. On the other hand, if the node failure occurs after the decision, the sensing  task of the network will be temporarily affected:  only during  the period of sensing until a new period starts.
+
+%The  energy consumption  and some other constraints  can easily  be  taken into account since the  sensors  can  update and  then  exchange their  information (including their residual energy) at the beginning of each period.  However, the pre-sensing  phases (Information  Exchange, Leader  Election, and  Decision) are energy  consuming for some  nodes, even  when they  do not  join the  network to monitor the area.
+
+ 
+
 
 
 
@@ -330,7 +332,7 @@ Obviously, in  that case, DESK and GAF have fewer active nodes since they have a
 %\subsection{Stopped simulation runs}
 %\label{ch5:sec:03:02:03}
 
-Figure~\ref{fig6} reports the cumulative  percentage of stopped simulations runs per round for 150 deployed nodes. This figure gives the  breakpoint for each method.  \\ \\ \\ \\
+Figure~\ref{fig6} reports the cumulative  percentage of stopped simulations runs per round for 150 deployed nodes. This figure gives the  breakpoint for each method.  
 DESK stops first,  after approximately 45~rounds, because it consumes the more energy by  turning on a large number of redundant  nodes during the sensing phase. GAF  stops secondly for the  same reason than  DESK.  MuDiLCO overcomes DESK and GAF because the  optimization process distributed on several subregions leads  to coverage  preservation and  so extends  the network  lifetime.  Let us
 emphasize that the  simulation continues as long as a network  in a subregion is still connected. \\
 
@@ -370,7 +372,7 @@ network sizes, for $Lifetime_{95}$ and $Lifetime_{50}$.
 
 The  results  show  that  MuDiLCO  is  the  most  competitive  from  the  energy consumption point of view.  The  other approaches have a high energy consumption due  to activating a  larger number  of redundant  nodes, as  well as  the energy consumed during  the different  status of the  sensor node. Among  the different versions of our protocol, the MuDiLCO-7  one consumes more energy than the other versions. This is  easy to understand since the bigger the  number of rounds and
 the number of  sensors involved in the integer program, the larger the time computation to solve the optimization problem. To improve the performances of MuDiLCO-7, we  should increase the  number of subregions  in order to  have fewer sensors to consider in the integer program.
-\\ \\ \\
+
 
 
  \item {{\bf Execution time}}
@@ -391,14 +393,15 @@ seconds (needed to solve optimization problem) for different values of $T$. The
 \end{figure} 
 
 As expected,  the execution time increases  with the number of  rounds $T$ taken into account to schedule the sensing phase. The times obtained for $T=1,3$ or $5$ seem bearable, but for $T=7$ they become quickly unsuitable for a sensor node, especially when  the sensor network size increases.   Again, we can notice that if we want  to schedule the nodes activities for a  large number of rounds,
-we need to choose a relevant number of subregions in order to avoid a complicated and cumbersome optimization.  On the one hand, a large value  for $T$ permits to reduce the  energy overhead due  to the three  pre-sensing phases, on  the other hand  a leader  node may  waste a  considerable amount  of energy  to  solve the optimization problem. \\
+we need to choose a relevant number of subregions in order to avoid a complicated and cumbersome optimization.  
 
+On the one hand, a large value  for $T$ permits to reduce the  energy overhead due  to the three  pre-sensing phases, on  the other hand  a leader  node may  waste a  considerable amount  of energy  to  solve the optimization problem. %\\ \\ \\ \\ \\ \\ \\
 
 \item {{\bf Network lifetime}}
 %\subsection{Network lifetime}
 %\label{ch5:sec:03:02:06}
 The next  two figures,  Figures~\ref{fig8}(a) and \ref{fig8}(b),  illustrate the network lifetime  for different network sizes,  respectively for $Lifetime_{95}$ and  $Lifetime_{50}$.  Both  figures show  that the  network  lifetime increases together with the  number of sensor nodes, whatever the  protocol, thanks to the node  density  which  results in  more  and  more  redundant  nodes that  can  be deactivated and thus save energy.  Compared to the other approaches, our MuDiLCO
-protocol  maximizes the  lifetime of  the network.   In particular,  the  gain in lifetime for a  coverage over 95\% is greater than 38\%  when switching from GAF to MuDiLCO-3. \\ \\ \\ 
+protocol  maximizes the  lifetime of  the network.   In particular,  the  gain in lifetime for a  coverage over 95\% is greater than 38\%  when switching from GAF to MuDiLCO-3.  
 
 \begin{figure}[h!]
 \centering
@@ -414,10 +417,11 @@ protocol  maximizes the  lifetime of  the network.   In particular,  the  gain i
 \end{figure}
 
 
-\end{enumerate} 
 The  slight decrease that can be observed  for MuDiLCO-7 in case of  $Lifetime_{95}$  with  large  wireless  sensor  networks  results  from  the difficulty  of the optimization  problem to  be solved  by the  integer program.
 This  point was  already noticed  in \ref{subsec:EC} devoted  to the
 energy consumption,  since network lifetime and energy  consumption are directly linked.
+\end{enumerate} 
+
 
 \section{Conclusion}
 \label{ch5:sec:05}
