X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/3d06a5c3f39989cad3f899ea07b088a5e8f3716b..de19a5ef179d0e0b0a56acf7549582147ba4b9c1:/CHAPITRE_01.tex?ds=inline

diff --git a/CHAPITRE_01.tex b/CHAPITRE_01.tex
index b49907c..58e5aff 100644
--- a/CHAPITRE_01.tex
+++ b/CHAPITRE_01.tex
@@ -420,7 +420,9 @@ Where $R_u$ is a measure of the uncertainty in sensor detection, $\alpha = d(s_i
 
 \end{enumerate}
 
-The coverage protocols have proposed in this dissertation use the binary disc sensing model as a sensing coverage model for each wireless sensor node in WSN.
+The coverage protocols proposed in this dissertation use the binary disc sensing model as a sensing coverage model for each wireless sensor node in WSN because we consider for each sensor a set of primary points and we assume that the sensing disk defined by a sensor is covered if all the primary points of this sensor are covered.
+
+%The coverage protocols have proposed in this dissertation use the binary disc sensing model as a sensing coverage model for each wireless sensor node in WSN.
 
 
 
@@ -430,12 +432,12 @@ The coverage protocols have proposed in this dissertation use the binary disc se
 \indent Several design issues should be considered in order to produce solutions for the coverage problems in WSNs. These design issues can be classified into~\cite{ref103}:
 
 \begin{enumerate}[(i)]
-\item $\textbf{Coverage Type}$ refers to determining what is it exactly that you are trying to cover. Typically, it may be required to monitor a whole area, observe a set of targets, or look for a breach of a barrier.
+\item $\textbf{Coverage Type}$ Is the WSN dedicated to monitor a whole area, to observe a set of targets, or to look for a breach of a barrier?
  
 \item $\textbf{Deployment Method}$ refers to the way by which the wireless sensor nodes are deployed over the target sensing field in order to build the wireless sensor network. Generally, the sensor nodes can be placed either deterministically or randomly in the target sensing field so as to construct the wireless sensor network~\cite{ref107}. The method of placement the sensor nodes can be selected based on the type of sensors, application, and the environment. In the deterministic placing, the deployment can be achieved in case of small number of sensor nodes and in friendly environment, whilst for a large number of sensor nodes or where the area of interest is inaccessible or hostile, a random placing is the choice. The sensor network can be either dense or sparse. The dense deployment is preferable when it is necessary to provide a security robustness in WSNs. On the other hand, the sparse deployment is used when the dense deployment is expensive or when the maximum coverage is performed by a less number of sensor nodes.
 
 
-\item $\textbf{Coverage Degree}$ refers to how many sensor nodes are required to cover a target or an area. This K-coverage means the point in the sensing field is covered by at least K sensor nodes. Some applications need a high reliability to achieve their tasks. Therefore, the sensing field is deployed densely so as to perform a K-coverage for this field. The simple coverage problem consists of a coverage degree equal to one (i.e., K=1), where every point in the sensing field is covered with at least one sensor.
+\item $\textbf{Coverage Degree}$ refers to how many sensor nodes are required to cover a target or an area. A point in the sensing field is said to be K-coverage by at least K sensor nodes. Some applications need a high reliability to achieve their tasks. Therefore, the sensing field is deployed densely so as to perform a K-coverage for this field. The simple coverage problem consists of a coverage degree equal to one (i.e., K=1), where every point in the sensing field is covered by at least one sensor.
 
 \item $\textbf{Coverage Ratio}$ is the percentage of the area of sensing field that fulfills the coverage degree of the application. If all the points in the sensing field are covered, the coverage ratio is $100\%$ and it can be called a complete coverage. Otherwise, it can be called as partial coverage.
 
@@ -449,11 +451,12 @@ The coverage protocols have proposed in this dissertation use the binary disc se
 
 \section{Energy Consumption Modeling} 
 \label{ch1:sec:9}
-\indent The WSNs have been received a lot of interests because the low energy consumption of the sensor nodes.  One of the most critical issues in WSNs is to reduce the energy consumption of the limited power battery of the sensor nodes so as to prolong the network lifetime as long as possible. In order to model the energy consumption, four states for a sensor node are used~\cite{ref140}:  transmission, reception, listening, and sleeping. In addition, two states should be taken into account: computation and sensed data acquisition. The main tasks of each of these states include:
+%\indent The WSNs have been received a lot of interests because the low energy consumption of the sensor nodes.  
+One of the most critical issues in WSNs is to reduce the energy consumption of the limited power battery of the sensor nodes so as to prolong the network lifetime as long as possible. In order to model the energy consumption, four states for a sensor node are used~\cite{ref140}:  transmission, reception, listening, and sleeping. In addition, two states should be taken into account: computation and sensed data acquisition. The main tasks of each of these states include:
 
 \begin{enumerate}[(i)]
 
-\item Computation: processing needed for clustering and executing any algorithm inside the sensor node.  The processing that required to physical communication and networking protocols is included in reception and transmission.
+\item Computation: processing needed for executing any algorithm inside the sensor node.  The processing that is required to physical communication and networking protocols is included in reception and transmission.
 
 \item Transmission:  processing for address determination, packetization, encoding, framing, and maybe queuing; supply for the baseband and RF circuitry.
 
@@ -474,7 +477,7 @@ The coverage protocols have proposed in this dissertation use the binary disc se
 
 %\subsection{Radio Energy Dissipation Model:}
 %\label{ch1:sec9:subsec1}
-\indent Since the communication unit is the most energy-consuming part of the sensor node; therefore, many authors are used the radio energy dissipation model that proposed in~\cite{ref109,ref110} as energy consumption model during the simulation and evaluation of their works in WSNs. Figure~\ref{RDM} shows the radio energy dissipation model.
+\indent The communication unit is the most energy-consuming part of the sensor node; many authors use the radio energy dissipation model proposed in~\cite{ref109,ref110} as energy consumption model. Figure~\ref{RDM} shows the radio energy dissipation model.
 \begin{figure}[h!]
 \centering
 \includegraphics[scale=0.4]{Figures/ch1/RDM.eps} 
@@ -482,7 +485,7 @@ The coverage protocols have proposed in this dissertation use the binary disc se
 \label{RDM}
 \end{figure}
 
-\indent In this model, the radio consumes an energy to execute the transmitter and the power amplifier. The receiver circuitry consumes an energy to run the radio electronics, as described in figure~\ref{RDM}.  The channel model can be either free space ($d^2$ power loss) or multipath fading ($d^4$ power loss), based on the distance between the transmitter and receiver. This power loss can be controlled by setting the power amplifier so that if the distance is less than a threshold, the free space ($\varepsilon_{fs}$) model is used (i.e., $\varepsilon_{amp}$ = $\varepsilon_{fs}$); Otherwise, the multipath ($\varepsilon_{mp}$) model is used (i.e., $\varepsilon_{amp}$ = $\varepsilon_{mp}$). Therefore, to transmit a k-bit packet with a distance d, the radio expends
+\indent In this model, the radio consumes energy to execute the transmitter and the power amplifier. The receiver circuitry consumes energy to run the radio electronics, as described in figure~\ref{RDM}.  The channel model can be either free space ($d^2$ power loss) or multipath fading ($d^4$ power loss), based on the distance between the transmitter and receiver. This power loss can be controlled by setting the power amplifier so that if the distance is less than a threshold, the free space ($\varepsilon_{fs}$) model is used (i.e., $\varepsilon_{amp}$ = $\varepsilon_{fs}$); Otherwise, the multipath ($\varepsilon_{mp}$) model is used (i.e., $\varepsilon_{amp}$ = $\varepsilon_{mp}$). Therefore, to transmit a k-bit packet with a distance d, the radio expends
 
 
 \begin{equation}
@@ -503,7 +506,7 @@ As well as to receive a k-bit packet, the radio expends
 
 The typical parameters are set as: $E_{elec}$ = 50 nJ/bit, $\varepsilon_{fs}$ = 10 pJ/bit/$m^2$, $\varepsilon_{mp}$ = 0.0013 pJ/bit/$m^4$. In addition, the energy for data aggregation is set as $E_{DA}$ = 5 nJ/bit.
 
-\indent The radio energy dissipation model have been considered only the energy, which is consumed by the communication part of the sensor node. However, in order to achieve a more accurate model, it is necessary to take into account the energy is consumed by the other parts inside the sensor node such as computation unit and sensing unit. 
+\indent The radio energy dissipation model considers only the energy consumed by the communication part of the sensor node. However, in order to achieve a more accurate model, it is necessary to take into account the energy consumed by other parts inside the sensor node such as computation unit and sensing unit. 
 
 %\subsection{Our Energy Consumption Model:}
 %\label{ch1:sec9:subsec2}
@@ -512,4 +515,4 @@ The typical parameters are set as: $E_{elec}$ = 50 nJ/bit, $\varepsilon_{fs}$ =
 \section{Conclusion}
 \label{ch1:sec:10}
 
-\indent In this chapter, an overview of the wireless sensor networks have been presented that shows our focus in this dissertation.  The structure of the typical wireless sensor network and the main components of the sensor nodes have been demonstrated. Several types of wireless sensor networks are described. Various fields of applications covering a wide spectrum for a WSNs including health, home, environmental, military, and industrial applications have been presented.  As demonstrated, since sensor nodes have limited battery life; since it is impossible to replace batteries, especially in remote and hostile environments; the limited power of a battery represents the critical challenge in WSNs. The main challenges in WSNs have explained; on the other hand, the energy efficient solutions have proposed in order to handle these challenges. Many energy efficient mechanisms have been illustrated, which are aimed to reduce the energy consumption by the different units of the wireless sensor nodes in WSNs. The definition of the network lifetime has been presented and in different contexts.  The problem of the coverage is explained, where constructing energy efficient coverage protocols one of the main scientific research challenges in WSNs. This chapter highlights the main design issues for the coverage problems that need to be considered in designing a coverage protocol for WSNs. In addition, the energy consumption Modeling have been demonstrated. 
+\indent In this chapter, an overview of the wireless sensor networks has been presented. Unlike traditional ad-hoc networks, WSNs are collaborative and very oriented toward a specific application domain. The structure of the typical wireless sensor network and the main components of the sensor nodes have been detailed. Several types of wireless sensor networks are described. Various fields of applications covering a wide spectrum for a WSNs including health, home, environmental, military, and industrial applications have been presented.  As shown, since sensor nodes have limited battery life; since it is impossible to replace batteries, especially in remote and hostile environments; the limited power of a battery represents the critical challenge in WSNs. The main challenges in WSNs have explained. Energy efficiency is the primary challenge to increase the network lifetime. Therefore, the energy efficient solutions have proposed in order to handle that challenge. Many energy efficient mechanisms have been illustrated, which are aimed to reduce the energy consumption of the different parts of the wireless sensor nodes in WSNs. The definition of the network lifetime has been presented and in different contexts.  The problem of the coverage in WSNs is explained.  One of the main scientific research challenges in WSNs is how to build energy efficient coverage protocols. This chapter highlights the main design issues for the coverage problems that need to be considered in designing a coverage protocol for WSNs. In addition, the energy consumption modeling have been illustrated. 
\ No newline at end of file
