X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/527e2e13b134e5c86779182bc5756daa144161c2..1e6c973630b57cc7cf78232de0f9c8b3bf0d334b:/CHAPITRE_05.tex

diff --git a/CHAPITRE_05.tex b/CHAPITRE_05.tex
index 94188d8..95ad64d 100644
--- a/CHAPITRE_05.tex
+++ b/CHAPITRE_05.tex
@@ -22,7 +22,7 @@ Compared to DiLCO protocol in chapter 4, in this one we study the possibility of
 
 
 The remainder of this chapter continues with section \ref{ch5:sec:02} where a detailed description of MuDiLCO Protocol is given. The next section describes the primary points based multiround coverage problem formulation  which is used to schedule the activation of sensors in multiple cover sets. Section \ref{ch5:sec:04} shows the simulation
-results. The chapter ends with a conclusion and some suggestions for further work.
+results. The chapter ends with a conclusion and some suggestions for further works.
 
 
  
@@ -32,7 +32,7 @@ results. The chapter ends with a conclusion and some suggestions for further wor
 \label{ch5:sec:02}
 %\noindent In this section, we introduce the MuDiLCO protocol which is distributed on each subregion in the area of interest. It 
 Like DiLCO, the MuDiLCO protocol is based on two energy-efficient
-mechanisms: subdividing the area of interest into several subregions (like cluster architecture) using divide and conquer method, where the sensor nodes cooperate within each subregion as independent group in order to achieve a network leader election; and sensor activity scheduling for maintaining the coverage and prolonging the network lifetime, which are applied periodically. MuDiLCO uses the same assumptions, primary point coverage and network models, than DiLCO, given in section \ref{ch4:sec:02:01} and \ref{ch4:sec:02:02}, respectively.
+mechanisms: subdividing the area of interest into several subregions (like a cluster architecture) using the divide and conquer method, where the sensor nodes cooperate within each subregion as independent group in order to achieve a network leader election. Sensor activity scheduling is used to maintain the coverage and to prolong the network lifetime, it is applied periodically. MuDiLCO uses the same assumptions, primary point coverage and network models, than DiLCO, given in section \ref{ch4:sec:02:01} and \ref{ch4:sec:02:02}, respectively.
 
  
 %\subsection{Background Idea and Algorithm}
@@ -41,7 +41,7 @@ mechanisms: subdividing the area of interest into several subregions (like clust
 
 As can be seen in Figure~\ref{fig2},  our protocol  works in  periods fashion, where  each is  divided  into 4  phases: Information~Exchange,  Leader~Election, Decision, and Sensing. 
 %The information exchange among wireless sensor nodes is described in chapter 4, section \ref{ch4:sec:02:03:01}. The leader election in each subregion is explained in chapter 4, section \ref{ch4:sec:02:03:02}, 
-The difference with MuDiLCO in that the elected leader in each subregion is for each period. In decision phase, each leader will solve an integer  program to select which  cover sets  will be activated in  the following  sensing phase  to cover the  subregion to  which it belongs.  The integer  program will produce $T$ cover sets,  one for each round. The leader will send an ActiveSleep  packet to each sensor in the subregion based on the algorithm's results, indicating if the sensor should be active or not in
+The difference with MuDiLCO in that the elected leader in each subregion is for each period. In the decision phase, each leader will solve an integer  program to select which  cover sets  will be activated in  the following  sensing phase  to cover the  subregion to  which it belongs.  The integer  program will produce $T$ cover sets,  one for each round. The leader will send an ActiveSleep  packet to each sensor in the subregion based on the algorithm's results, indicating if the sensor should be active or not in
 each round  of the  sensing phase. Each sensing phase is itself divided into $T$ rounds and for each round a set of sensors (a cover set) is responsible for the sensing task. 
 %Each sensor node in the subregion will receive an ActiveSleep packet from leader, informing it to stay awake or to go to sleep for  each round of the sensing  phase. 
 Algorithm~\ref{alg:MuDiLCO}, which will be  executed by each node at the beginning  of a period, explains  how the ActiveSleep packet is obtained. In this way, a multiround optimization  process is performed  during each
@@ -53,7 +53,7 @@ period  after  Information~Exchange  and  Leader~Election phases,  in  order to
 \end{figure} 
 
 
-This protocol minimizes the impact of unexpected node failure (not due to batteries running out of energy), because it works in periods. On the one hand, if a node failure is detected before making the decision, the node will not participate during this phase, and, on the other hand, if the node failure occurs after the decision, the sensing  task of the network will be temporarily affected:  only during  the period of sensing until a new period starts.
+This protocol minimizes the impact of unexpected node failure (not due to batteries running out of energy), because it works in periods. On the one hand, if a node failure is detected before making the decision, the node will not participate during this phase. On the other hand, if the node failure occurs after the decision, the sensing  task of the network will be temporarily affected:  only during  the period of sensing until a new period starts.
 
 The  energy consumption  and some other constraints  can easily  be  taken into account since the  sensors  can  update and  then  exchange their  information (including their residual energy) at the beginning of each period.  However, the pre-sensing  phases (Information  Exchange, Leader  Election, and  Decision) are energy  consuming for some  nodes, even  when they  do not  join the  network to monitor the area.
 
@@ -146,7 +146,7 @@ We define the Overcoverage variable $\Theta_{t,p}$ as
     & \mbox{is not covered during round $t$,}\\
   \left( \sum_{j \in J} \alpha_{jp} * X_{tj} \right)- 1 & \mbox{otherwise.}\\
 \end{array} \right.
-\label{eq13} 
+\label{eq133} 
 \end{equation}
 More  precisely, $\Theta_{t,p}$  represents the  number of  active  sensor nodes
 minus  one  that  cover  the  primary  point $p$  during  round  $t$.   The
@@ -158,7 +158,7 @@ U_{t,p} = \left \{
   1 &\mbox{if the primary point $p$ is not covered during round $t$,} \\
   0 & \mbox{otherwise.}\\
 \end{array} \right.
-\label{eq14} 
+\label{eq1114} 
 \end{equation}
 
 Our coverage optimization problem can then be formulated as follows
@@ -291,7 +291,7 @@ indicate the energy consumed by the whole network in round $t$ of the sensing ph
 \end{frame}
 
 \subsection{Results Analysis and Comparison }
-\label{ch5:sec:04:02}
+\label{ch5:sec:04:03}
 
 
 \begin{enumerate}[i)]
@@ -441,8 +441,8 @@ energy consumption,  since network lifetime and energy  consumption are directly
 \section{Conclusion}
 \label{ch5:sec:05}
 
-We have addressed the problem of the coverage and of the lifetime optimization in wireless  sensor networks.  This is a key  issue as  sensor nodes  have limited resources in terms of memory, energy, and computational power. To cope with this problem,  the field  of sensing  is divided  into smaller subregions  using the concept of divide-and-conquer method, and  then  we propose  a protocol  which optimizes coverage  and lifetime performances in each  subregion.  Our protocol,
-called MuDiLCO (Multiround  Distributed Lifetime Coverage Optimization) combines two  efficient techniques:  network leader election  and   sensor  activity scheduling. The activity  scheduling in each subregion  works in periods,  where each period consists of four  phases: (i) Information exchange, (ii)  Leader election, (iii) Decision phase to plan the activity  of the sensors over $T$ rounds, (iv) Sensing phase itself divided into T rounds.
+%We have addressed the problem of the coverage and of the lifetime optimization in wireless  sensor networks.  This is a key  issue as  sensor nodes  have limited resources in terms of memory, energy, and computational power. To cope with this problem,  the field  of sensing  is divided  into smaller subregions  using the concept of divide-and-conquer method, and  then  we propose  a protocol  which optimizes coverage  and lifetime performances in each  subregion.  
+In this chapter, we have presented a protocol, called MuDiLCO (Multiround  Distributed Lifetime Coverage Optimization) that combines two  efficient techniques:  network leader election  and sensor activity scheduling. The activity scheduling in each subregion  works in periods, where each period consists of four  phases: (i) Information exchange, (ii)  Leader election, (iii) Decision phase to plan the activity  of the sensors over $T$ rounds, (iv) Sensing phase itself divided into T rounds.
 
 Simulations results show the  relevance of the proposed  protocol in  terms of lifetime, coverage  ratio, active  sensors ratio, energy  consumption, execution time. Indeed,  when dealing with  large wireless sensor networks,  a distributed approach, like  the one we  propose, allows to reduce the difficulty of  a single global optimization problem by partitioning it into many smaller problems, one per subregion, that can be solved  more easily. Nevertheless, results also show that it is not possible to plan the activity of sensors over too many rounds because the resulting optimization problem leads to too high-resolution times and thus to an excessive energy consumption. Compared with DiLCO, it is clear that MuDiLCO improves the network lifetime especially for the dense network, but it is  less robust than DiLCO under sensor nodes failures. Therefore, choosing the number of rounds $T$ depends on the type of application the WSN is deployed for. 
 
