X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/7514818a403dda39ca986485675952cd8f78932e..e8beaffc3d795b3bf326898f4c0df08d8eaea6c1:/CHAPITRE_04.tex

diff --git a/CHAPITRE_04.tex b/CHAPITRE_04.tex
index 3e691b7..09b6595 100644
--- a/CHAPITRE_04.tex
+++ b/CHAPITRE_04.tex
@@ -344,38 +344,27 @@ The modeling language for Mathematical Programming (AMPL)~\cite{AMPL} is  employ
 
 \indent For our energy consumption model, we refer to the sensor node Medusa~II which uses an Atmel's  AVR ATmega103L microcontroller~\cite{ref112}. The typical architecture  of a  sensor  is composed  of four  subsystems: the  MCU subsystem which is capable of computation, communication subsystem (radio) which is responsible  for transmitting/receiving messages, the  sensing subsystem that collects  data, and  the  power supply  which  powers the  complete sensor  node \cite{ref112}. Each  of the first three subsystems  can be turned on or  off depending on  the current status  of the sensor.   Energy consumption (expressed in  milliWatt per second) for  the different status of  the sensor is summarized in Table~\ref{table1}.
 
-\begin{table}[ht]
-\caption{Energy Consumption Model}
-% title of Table
+\begin{table}[h]
 \centering
-% used for centering table
-\begin{tabular}{|c|c|c|c|c|}
-% centered columns (4 columns)
-      \hline
-%inserts double horizontal lines
-Sensor status & MCU & Radio & Sensing & Power (mW) \\ [0.5ex]
-\hline
-% inserts single horizontal line
-LISTENING & on & on & on & 20.05 \\
-% inserting body of the table
-\hline
-ACTIVE & on & off & on & 9.72 \\
-\hline
-SLEEP & off & off & off & 0.02 \\
-\hline
-COMPUTATION & on & on & on & 26.83 \\
-%\hline
-%\multicolumn{4}{|c|}{Energy needed to send/receive a 1-bit} & 0.2575\\
- \hline
+\caption{Power consumption values}
+\label{tab:EC}
+\begin{tabular}{|l||cccc|}
+  \hline
+  {\bf Sensor status} & MCU & Radio & Sensor & {\it Power (mW)} \\
+  \hline
+  LISTENING & On & On & On & 20.05 \\
+  ACTIVE & On & Off & On & 9.72 \\
+  SLEEP & Off & Off & Off & 0.02 \\
+  COMPUTATION & On & On & On & 26.83 \\
+  \hline
+  \multicolumn{4}{|l}{Energy needed to send or receive a 2-bit content message} & 0.515 \\
+  \hline
 \end{tabular}
-
-\label{table1}
-% is used to refer this table in the text
 \end{table}
 
 \indent For the sake of simplicity we ignore  the energy needed to turn on the radio, to start up the sensor node, to move from one status to another, etc. Thus, when a sensor becomes active (i.e., it has already received its status from leader), it can turn  its radio  off to  save battery. DiLCO uses two types of packets
 for communication. The size of the INFO packet and ActiveSleep packet
-are 112 bits and 16 bits respectively. The value of energy spent to send a 1-bit-content message is  obtained by using  the equation in ~\cite{ref112} to calculate  the energy cost for transmitting  messages and  we propose  the same value for receiving the packets. The energy  needed to send or receive a 1-bit packet is equal to $0.2575~mW$.
+are 112 bits and 16 bits respectively. The value of energy spent to send a 2-bit-content message is  obtained by using  the equation in ~\cite{ref112} to calculate  the energy cost for transmitting  messages and  we propose  the same value for receiving the packets. The energy  needed to send or receive a 1-bit packet is equal to $0.2575~mW$.
 
 %We have used an energy consumption model, which is presented in chapter 1, section \ref{ch1:sec9:subsec2}. 
 
