X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/906798a11837d58c5c67e336737c965f10f52362..396b3d0c06b453c33e2a3a7e0aa81187f1df9880:/CHAPITRE_06.tex

diff --git a/CHAPITRE_06.tex b/CHAPITRE_06.tex
index 66f0e6a..ad7bd09 100644
--- a/CHAPITRE_06.tex
+++ b/CHAPITRE_06.tex
@@ -209,7 +209,7 @@ The sensors  inside a same  region cooperate to  elect a leader.   The selection
 \item larger  remaining energy;
 \item and then  in case  of equality,  larger index.
 \end{enumerate}
-Once chosen, the leader collects information  to formulate and solve the integer program  which allows  to construct  the set  of active  sensors in  the sensing stage. \textcolor{blue}{The flowchart of PeCO protocol executed in each sensor node is presented in Figure \ref{flow6}.} 
+Once chosen, the leader collects information  to formulate and solve the integer program  which allows  to construct  the set  of active  sensors in  the sensing stage. The flowchart of PeCO protocol executed in each sensor node is presented in Figure \ref{flow6}.
 
 \begin{figure}[ht!]
 \centering
