X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/906798a11837d58c5c67e336737c965f10f52362..refs/heads/master:/CHAPITRE_05.tex?ds=inline

diff --git a/CHAPITRE_05.tex b/CHAPITRE_05.tex
index 7cf8725..918ec90 100644
--- a/CHAPITRE_05.tex
+++ b/CHAPITRE_05.tex
@@ -92,7 +92,7 @@ The difference with MuDiLCO in that the elected leader in each subregion is for
 each round  of the  sensing phase. Each sensing phase is itself divided into $T$ rounds and for each round a set of sensors (a cover set) is responsible for the sensing task. 
 %Each sensor node in the subregion will receive an ActiveSleep packet from leader, informing it to stay awake or to go to sleep for  each round of the sensing  phase. 
 Algorithm~\ref{alg:MuDiLCO}, which will be  executed by each node at the beginning  of a period, explains  how the ActiveSleep packet is obtained. In this way, a multiround optimization  process is performed  during each
-period  after  Information~Exchange  and  Leader~Election phases,  in  order to produce $T$ cover sets that will take the mission of sensing for $T$ rounds. \textcolor{blue}{The flowchart of MuDiLCO protocol executed in each sensor node is presented in Figure \ref{flow5}.} 
+period  after  Information~Exchange  and  Leader~Election phases,  in  order to produce $T$ cover sets that will take the mission of sensing for $T$ rounds. The flowchart of MuDiLCO protocol executed in each sensor node is presented in Figure \ref{flow5}.
 
 \begin{figure}[ht!]
 \centering
