X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/9eaa0b57db7b53eb9338a3fe8205215cdb0f9683..df0ded57ac60ab03ead82d37326459a25812634a:/CHAPITRE_06.tex?ds=sidebyside

diff --git a/CHAPITRE_06.tex b/CHAPITRE_06.tex
index 33c8fa3..0ea4365 100644
--- a/CHAPITRE_06.tex
+++ b/CHAPITRE_06.tex
@@ -209,7 +209,14 @@ The sensors  inside a same  region cooperate to  elect a leader.   The selection
 \item larger  remaining energy;
 \item and then  in case  of equality,  larger index.
 \end{enumerate}
-Once chosen, the leader collects information  to formulate and solve the integer program  which allows  to construct  the set  of active  sensors in  the sensing stage.
+Once chosen, the leader collects information  to formulate and solve the integer program  which allows  to construct  the set  of active  sensors in  the sensing stage. \textcolor{blue}{The flow chart of PeCO protocol that executed in each sensor node is presented in \ref{flow6}.} 
+
+\begin{figure}[ht!]
+\centering
+\includegraphics[scale=0.45]{Figures/ch6/Algo3.pdf} % 70mm
+\caption{The flow chart of PeCO protocol.}
+\label{flow6}
+\end{figure} 
 
 
 \section{Perimeter-based Coverage Problem Formulation}
