X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/c8aeaf03fab9cb2dd9e45068f1cb29c3ed7984db..7976cef0966cf4550fcfd57c22cebce39f5fc3c3:/INTRODUCTION.tex?ds=inline

diff --git a/INTRODUCTION.tex b/INTRODUCTION.tex
index 847f097..715cab3 100644
--- a/INTRODUCTION.tex
+++ b/INTRODUCTION.tex
@@ -43,7 +43,7 @@ The main contributions in this dissertation concentrate on designing distributed
 \item We devise a framework to schedule nodes to be activated alternatively such that the network lifetime is prolonged  while ensuring that a certain level of coverage is preserved. A key idea in our framework is  to exploit a spatial-temporal subdivision. On the one hand, the area of interest is divided into several smaller subregions.On the other hand, the timeline is divided into periods of equal length. In each subregion, the sensor nodes will cooperatively choose a  leader which will schedule  nodes' activities, and this grouping of sensors is similar to typical cluster architecture.
 
 
-\item We design, called the Distributed Lifetime Coverage Optimization (DILCO) protocol, which maintains the coverage and improves the lifetime in WSNs. DILCO protocol is presented in chapter 4. It is an extension of our approach introduced in \cite{ref159}. In \cite{ref159}, the protocol is deployed over only two subregions. In DILCO protocol, the area of interest is first divided into subregions using a divide-and-conquer algorithm and an activity scheduling for sensor nodes is then planned by the elected leader in each subregion. In fact, the nodes in a subregion can be seen as a cluster where each node sends sensing data to the cluster head or the sink node. Furthermore, the activities in a subregion/cluster can continue even if another cluster stops due to too many node failures. DiLCO protocol considers periods, where a period starts with a discovery phase to exchange information between sensors of the same subregion, in order to choose in a suitable manner a sensor node (the leader) to carry out the coverage strategy. In each subregion, the activation of the sensors for the sensing phase of the current period is obtained by solving an integer program. The resulting activation vector is broadcasted by the leader to every node of its subregion.
+\item We design a protocol, called the Distributed Lifetime Coverage Optimization (DILCO) protocol, which maintains the coverage and improves the lifetime in WSNs. DILCO protocol is presented in chapter 4. It is an extension of our approach introduced in \cite{ref159}. In \cite{ref159}, the protocol is deployed over only two subregions. In DILCO protocol, the area of interest is first divided into subregions using a divide-and-conquer algorithm and an activity scheduling for sensor nodes is then planned by the elected leader in each subregion. In fact, the nodes in a subregion can be seen as a cluster where each node sends sensing data to the cluster head or the sink node. Furthermore, the activities in a subregion/cluster can continue even if another cluster stops due to too many node failures. DiLCO protocol considers periods, where a period starts with a discovery phase to exchange information between sensors of the same subregion, in order to choose in a suitable manner a sensor node (the leader) to carry out the coverage strategy. In each subregion, the activation of the sensors for the sensing phase of the current period is obtained by solving an integer program. The resulting activation vector is broadcasted by the leader to every node of its subregion.
 
 \item %We extend our work that explained in chapter 4 and present a generalized framework that can be applied to provide the cover sets of all rounds in each period. 
 The MuDiLCO protocol for Multiround Distributed Lifetime Coverage Optimization protocol, presented in chapter 5, is an extension of the approach introduced in chapter 4. In DiLCO protocol, the activity scheduling based optimization is planned for each subregion periodically only for one sensing round. Whilst, we study the possibility of dividing the sensing phase into multiple rounds. In fact, we make a multiround optimization, while it was a single round optimization in our previous contribution.
