X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/UIC2013.git/blobdiff_plain/763e6024a4df2631498b5b9e77063abdf69dc9bc..e56d6e1ea749e2e2e5a14854e6b82c16939dd51f:/bare_conf.tex?ds=sidebyside

diff --git a/bare_conf.tex b/bare_conf.tex
index c1003b8..a6cc277 100755
--- a/bare_conf.tex
+++ b/bare_conf.tex
@@ -430,7 +430,7 @@ active mode.
 This  step includes choosing  the Wireless  Sensor Node  Leader (WSNL)
 which  will  be  responsible  of executing  coverage  algorithm.  Each
 subregion  in  the   area  of  interest  will  select   its  own  WSNL
-independently  for each  round.  All the  sensor  nodes cooperates  to
+independently  for each  round.  All the  sensor  nodes cooperate  to
 select WSNL.  The nodes in the  same subregion will  select the leader
 based on  the received  information from all  other nodes in  the same
 subregion.  The selection criteria  in order  of priority  are: larger
@@ -450,7 +450,7 @@ Active  sensors  in the  round  will  execute  their sensing  task  to
 preserve maximal  coverage in the  region of interest. We  will assume
 that the cost  of keeping a node awake (or sleep)  for sensing task is
 the same  for all wireless sensor  nodes in the  network.  Each sensor
-will  receive an  Active-Sleep packet  from WSNL  telling him  to stay
+will  receive an  Active-Sleep packet  from WSNL  informing it  to stay
 awake or  go sleep  for a time  equal to  the period of  sensing until
 starting a new round.
 
@@ -615,7 +615,7 @@ X_{j} \in \{0,1\}, &\forall j \in J
 \right.
 \end{equation}
 \begin{itemize}
-\item  $X_{j}$ :  indicates  whether  or not  sensor  $j$ is  actively
+\item  $X_{j}$ :  indicates  whether  or not  the sensor  $j$ is  actively
   sensing in the round (1 if yes and 0 if not);
 \item $\Theta_{p}$  : {\it overcoverage}, the number  of sensors minus
   one that are covering point $p$;
