X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/UIC2013.git/blobdiff_plain/c174b7277e5ba9b166983f25094db53a92de21f2..0ffd0e6c8834d66f5f7c08ad1752ad0879b8d791:/bare_conf.tex

diff --git a/bare_conf.tex b/bare_conf.tex
index c0cef5a..959f692 100755
--- a/bare_conf.tex
+++ b/bare_conf.tex
@@ -71,7 +71,7 @@ Election, (iii)~Decision,  and (iv)~Sensing.  The  decision process is
 carried  out  by  a  leader  node which  solves  an  integer  program.
 Simulation  results show that  the proposed  approach can  prolong the
 network lifetime and improve the coverage performance.
-\end{abstract*&^@!U&*T@}
+\end{abstract}
 
 %\keywords{Area Coverage, Wireless Sensor Networks, lifetime Optimization, Distributed Protocol.}
  
@@ -944,7 +944,7 @@ subdividing the sensing field  into many subregions, which are managed
 independently and simultaneously, is the most relevant way to maximize
 the lifetime of a network.
 
-\section{Conclusion and future forks}
+\section{Conclusion and Future Works}
 \label{sec:conclusion}
 
 In this paper, we have  addressed the problem of the coverage and the lifetime
