X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/book_gpu.git/blobdiff_plain/17bff40b83bcdcc39769f9e59c70ffae1c525b72..0f26b548f3029a96eafd6667024aabe2b36e464b:/BookGPU/Chapters/chapter16/gpu.tex

diff --git a/BookGPU/Chapters/chapter16/gpu.tex b/BookGPU/Chapters/chapter16/gpu.tex
index 26bd536..623ac81 100644
--- a/BookGPU/Chapters/chapter16/gpu.tex
+++ b/BookGPU/Chapters/chapter16/gpu.tex
@@ -160,7 +160,7 @@ period in order to solve a Newton update.
 At each time step, SPICE\index{SPICE} has
 to linearize device models, stamp matrix elements
 into MNA (short for modified nodal analysis\index{modified nodal analysis, or MNA}) matrices,
-and solve circuit equations in its inner Newton iteration\index{Newton iteration}.
+and solve circuit equations in its inner Newton iteration\index{iterative method!Newton iteration}.
 When convergence is attained,
 circuit states are saved and then next time step begins.
 This is also the time when we store the needed matrices
