X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/dmems12.git/blobdiff_plain/68ef101fa4f71c2911e9ffa93ceb5e07afb4af88..5bd43a57b7e5c885d77aac6dceea8cc19f2cfaea:/dmems12.tex?ds=inline

diff --git a/dmems12.tex b/dmems12.tex
index 51d7344..423b0f7 100644
--- a/dmems12.tex
+++ b/dmems12.tex
@@ -1,8 +1,9 @@
-\documentclass[12pt]{article}
+
+\documentclass[10pt, conference, compsocconf]{IEEEtran}
 %\usepackage{latex8}
 %\usepackage{times}
-\usepackage[latin1]{inputenc}
-\usepackage[cyr]{aeguill}
+\usepackage[utf8]{inputenc}
+%\usepackage[cyr]{aeguill}
 %\usepackage{pstricks,pst-node,pst-text,pst-3d}
 %\usepackage{babel}
 \usepackage{amsmath}
@@ -24,29 +25,38 @@
 
 \newcommand{\tab}{\ \ \ }
 
-%%%%%%%%%%%%%%%%%%%%%%%%%%%% my bib path.
+
+
+\begin{document}
+
+
+%% \author{\IEEEauthorblockN{Authors Name/s per 1st Affiliation (Author)}
+%% \IEEEauthorblockA{line 1 (of Affiliation): dept. name of organization\\
+%% line 2: name of organization, acronyms acceptable\\
+%% line 3: City, Country\\
+%% line 4: Email: name@xyz.com}
+%% \and
+%% \IEEEauthorblockN{Authors Name/s per 2nd Affiliation (Author)}
+%% \IEEEauthorblockA{line 1 (of Affiliation): dept. name of organization\\
+%% line 2: name of organization, acronyms acceptable\\
+%% line 3: City, Country\\
+%% line 4: Email: name@xyz.com}
+%% }
+
 
 
 \title{Using FPGAs for high speed and real time cantilever deflection estimation}
+\author{\IEEEauthorblockN{RaphaÃ«l Couturier\IEEEauthorrefmark{1}, StÃ©phane Domas\IEEEauthorrefmark{1}, GwenhaÃ«l Goavec-Merou\IEEEauthorrefmark{2} and Michel Lenczner\IEEEauthorrefmark{2}}
+\IEEEauthorblockA{\IEEEauthorrefmark{1}FEMTO-ST, DISC, University of Franche-Comte, Belfort, France\\
+\{raphael.couturier,stephane.domas\}@univ-fcomte.fr}
+\IEEEauthorblockA{\IEEEauthorrefmark{2}FEMTO-ST, Time-Frequency, University of Franche-Comte, BesanÃ§on, France\\
+\{michel.lenczner@utbm.fr,gwenhael.goavec@trabucayre.com}
+}
+
+
 
-\author{ Raphaël COUTURIER\\
-Laboratoire d'Informatique 
-de l'Universit\'e de  Franche-Comt\'e, \\
-BP 527, \\
-90016~Belfort CEDEX, France\\
- \and Stéphane Domas\\
-Laboratoire d'Informatique 
-de l'Universit\'e de  Franche-Comt\'e, \\
-BP 527, \\
-90016~Belfort CEDEX, France\\
- \and Gwenhaël Goavec\\
-??
-?? \\
-??, \\
-??\\}
 
 
-\begin{document}
 
 \maketitle
 
@@ -122,7 +132,7 @@ consider the camera actually in use, an exposition time of 2.5ms for
 $1024\times 1204$ pixels seems the minimum that can be reached. For a
 $10\times 10$ cantilever array, if we neglect the time to extract
 pixels, it implies that computing the deflection of a single
-cantilever should take less than 25$µ$s, thus 12.5$µ$s by phase.\\
+cantilever should take less than 25$\mu$s, thus 12.5$\mu$s by phase.\\
 
 In fact, this timing is a very hard constraint. Let consider a very
 small programm that initializes twenty million of doubles in memory
@@ -135,7 +145,7 @@ $3000$ operations.
 
 %% to be continued ...
 
-%% à faire : timing de l'algo spline en C avec atan et tout le bordel.
+%% ï¿½ faire : timing de l'algo spline en C avec atan et tout le bordel.
 
 
 
