X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/hpcc2014.git/blobdiff_plain/645f3921415c716f3c2185090bd32a5d48861879..c3bfcd6a7a6c9b0dcb1bcdc52facec1fe257f658:/hpcc.tex

diff --git a/hpcc.tex b/hpcc.tex
index 1179edb..c2f5a1b 100644
--- a/hpcc.tex
+++ b/hpcc.tex
@@ -259,7 +259,7 @@ their bandwidth and latency, and the routing strategy.  The simulated running
 time of the application is computed according to these properties.
 
 To compute the durations of the operations in the simulated world, and to take
-into account resource sharing (e.g.  bandwith sharing between competiting
+into account resource sharing (e.g. bandwidth sharing between competing
 communications), SimGrid uses a fluid model.  This allows to run relatively fast
 simulations, while still keeping accurate
 results~\cite{bedaride:hal-00919507,tomacs13}.  Moreover, depending on the
