X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/hpcc2014.git/blobdiff_plain/77214ec707f5ea85e7e3a85531991841bf182b75..9e58442a55b1f2eda6edb277b367dc4e34f1fa1e:/hpcc.tex

diff --git a/hpcc.tex b/hpcc.tex
index 3d92065..b857d5c 100644
--- a/hpcc.tex
+++ b/hpcc.tex
@@ -152,7 +152,7 @@ SimGrid toolkit~\cite{SimGrid}). Second, we confirm the effectiveness of
 asynchronous mode algorithms by comparing their performance with the synchronous
 mode. More precisely, we had implemented a program for solving large
 non-symmetric linear system of equations by numerical method GMRES (Generalized
-Minimal Residual) []\AG[]{[]?}. We show, that with minor modifications of the
+Minimal Residual) []\AG[]{[]?}.\LZK{ProblÃ¨me traitÃ© dans le papier est symÃ©trique ou asymÃ©trique? (Poisson 3D symÃ©trique?)} We show, that with minor modifications of the
 initial MPI code, the SimGrid toolkit allows us to perform a test campaign of a
 real AIAC application on different computing architectures. The simulated
 results we obtained are in line with real results exposed in ??\AG[]{??}.
@@ -555,10 +555,14 @@ lat latency, \dots{}).
 	\item Maximum number of internal and external iterations;
 	\item Internal and external precisions;
 	\item Matrix size $N_x$, $N_y$ and $N_z$;
+<<<<<<< HEAD
 	\item Matrix diagonal value: \np{6.0};
 	\item Matrix Off-diagonal value: \np{-1};
 	 \LZK{Off-diagonal values? (-1?)}
 	 \CER{oui}
+=======
+	\item Matrix diagonal value: \np{6.0}, \LZK{Off-diagonal values? (-1.0?)}
+>>>>>>> 5fb6769d88c1720b6480a28521119ef010462fa6
 	\item Execution Mode: synchronous or asynchronous.
 \end{itemize}
 
@@ -628,6 +632,8 @@ demonstrated an original solution to optimize the use of a simulation
 tool to run efficiently an iterative parallel algorithm in asynchronous 
 mode in a grid architecture. 
 
+\LZK{Perspectives???}
+
 \section*{Acknowledgment}
 
 This work is partially funded by the Labex ACTION program (contract ANR-11-LABX-01-01).
