X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/loba-papers.git/blobdiff_plain/2567705429f776512834d21c2e1e6e674d0057e2..ccdcd0ac01b39dae92f6c456577fafdb046a36bd:/loba-besteffort/loba-besteffort.tex?ds=sidebyside

diff --git a/loba-besteffort/loba-besteffort.tex b/loba-besteffort/loba-besteffort.tex
index 88ad560..c387ad6 100644
--- a/loba-besteffort/loba-besteffort.tex
+++ b/loba-besteffort/loba-besteffort.tex
@@ -346,7 +346,7 @@ information of the load they will receive, so they can take it into account.
 
 In order to test and validate our approaches, we wrote a simulator
 using the SimGrid
-framework~\cite{simgrid.web,casanova+legrand+quinson.2008.simgrid}.  This
+framework~\cite{simgrid.web,casanova+giersch+legrand+al.2014.simgrid}.  This
 simulator, which consists of about 2,700 lines of C++, allows to run
 the different load-balancing strategies under various parameters, such
 as the initial distribution of load, the interconnection topology, the
@@ -382,7 +382,7 @@ For the sake of simplicity, a few details were voluntary omitted from
 these descriptions.  For an exhaustive presentation, we refer to the
 actual source code that was used for the experiments%
 \footnote{As mentioned before, our simulator relies on the SimGrid
-  framework~\cite{casanova+legrand+quinson.2008.simgrid}.  For the
+  framework~\cite{casanova+giersch+legrand+al.2014.simgrid}.  For the
   experiments, we used a pre-release of SimGrid 3.7 (Git commit
   67d62fca5bdee96f590c942b50021cdde5ce0c07, available from
   \url{https://gforge.inria.fr/scm/?group_id=12})}, and which is
