X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/loba-papers.git/blobdiff_plain/a63036f3425d8303146d21053b097d533b3a6521..59636878becb2087601db617b593fd3f35181655:/loba-besteffort/loba-besteffort.tex

diff --git a/loba-besteffort/loba-besteffort.tex b/loba-besteffort/loba-besteffort.tex
index 03cb38c..3ccb2b0 100644
--- a/loba-besteffort/loba-besteffort.tex
+++ b/loba-besteffort/loba-besteffort.tex
@@ -347,7 +347,7 @@ information of the load they will receive, so they can take in into account.
 
 In order to test and validate our approaches, we wrote a simulator
 using the SimGrid
-framework~\cite{casanova+legrand+quinson.2008.simgrid}.  This
+framework~\cite{simgrid.web,casanova+legrand+quinson.2008.simgrid}.  This
 simulator, which consists of about 2,700 lines of C++, allows to run
 the different load-balancing strategies under various parameters, such
 as the initial distribution of load, the interconnection topology, the
