X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/loba-papers.git/blobdiff_plain/faef9adf00e740ce6fa28da521a29006b1cf6ac5..3a7899b35652f292727ce064ddf00c71717863be:/supercomp11/supercomp11.tex

diff --git a/supercomp11/supercomp11.tex b/supercomp11/supercomp11.tex
index 3010b1b..01ca4f7 100644
--- a/supercomp11/supercomp11.tex
+++ b/supercomp11/supercomp11.tex
@@ -29,12 +29,12 @@
 }
 
 \institute{R. Couturier \and A. Giersch \at
-              LIFC, University of Franche-ComtÃ©, Belfort, France \\
+              FEMTO-ST, University of Franche-ComtÃ©, Belfort, France \\
               % Tel.: +123-45-678910\\
               % Fax: +123-45-678910\\
               \email{%
-                raphael.couturier@univ-fcomte.fr,
-                arnaud.giersch@univ-fcomte.fr}
+                raphael.couturier@femto-st.fr,
+                arnaud.giersch@femto-st.fr}
 }
 
 \maketitle
@@ -492,7 +492,7 @@ This gives us as many as $4\times 2\times 2 = 16$ different strategies.
 
 \paragraph{Configurations}
 
-In order to show the behaviour of the different strategies in different
+In order to show the behavior of the different strategies in different
 settings, we simulated the executions on two sorts of platforms.  These two
 sorts of platforms differ by their underlaid network topology.  On the one hand,
 we have homogeneous platforms, modeled as a cluster.  On the other hand, we have
@@ -514,10 +514,10 @@ nodes: 16, 64, 256, and 1024 nodes.
 The distributed processes of the application were then logically organized along
 three possible topologies: a line, a torus or an hypercube.  We ran tests where
 the total load was initially on an only node (at one end for the line topology),
-and other tests where the load was initially randomly distributed accross all
+and other tests where the load was initially randomly distributed across all
 the participating nodes.
 
-For each of the preceding configuration, we finally had to cohose the
+For each of the preceding configuration, we finally had to choose the
 computation and communication costs of a load unit.  We chose them, such as to
 have three different computation over communication cost ratios, and hence model
 three different kinds of applications:
@@ -611,4 +611,4 @@ Taille : 10 100 trÃ¨s gros
 
 % LocalWords:  RaphaÃ«l Couturier Arnaud Giersch Abderrahmane Sider Franche ij
 % LocalWords:  Bertsekas Tsitsiklis SimGrid DASUD ComtÃ© BÃ©jaÃ¯a asynchronism ji
-% LocalWords:  ik isend irecv CortÃ©s et al chan ctrl fifo
+% LocalWords:  ik isend irecv CortÃ©s et al chan ctrl fifo Makhoul
