X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/mpi-energy2.git/blobdiff_plain/054bc9f5e26028cd84aa816c5c06ed131959fdde..8c643c738580db77edb260d118e0a2dc4af78ab2:/Heter_paper.tex?ds=sidebyside

diff --git a/Heter_paper.tex b/Heter_paper.tex
index 9d743db..ca66e17 100644
--- a/Heter_paper.tex
+++ b/Heter_paper.tex
@@ -63,8 +63,7 @@
     Arnaud Giersch
   } 
   \IEEEauthorblockA{%
-    FEMTO-ST Institute\\
-    University of Franche-ComtÃ©\\
+    FEMTO-ST Institute, University of Franche-Comte\\
     IUT de Belfort-MontbÃ©liard,
     19 avenue du MarÃ©chal Juin, BP 527, 90016 Belfort cedex, France\\
     % Telephone: \mbox{+33 3 84 58 77 86}, % RaphaÃ«l
@@ -83,8 +82,7 @@ platforms many techniques have been  used. Dynamic voltage and frequency scaling
 consumption.  However,  lowering the  frequency  of  a  CPU might  increase  the
 execution  time of  an application  running on  that processor.   Therefore, the
 frequency that  gives the best tradeoff  between the energy  consumption and the
-performance of an application must be selected.
-
+performance of an application must be selected.\\
 In this  paper, a new  online frequencies selecting algorithm  for heterogeneous
 platforms is presented.   It selects the frequency which tries  to give the best
 tradeoff  between  energy saving  and  performance  degradation,  for each  node
