X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/mpi-energy2.git/blobdiff_plain/2133c99a59a380205e2ebf91377e21251f84593e..d509f4d19eb0a9dfb0cb8fcc367e63e0e172fd42:/Heter_paper.tex?ds=inline

diff --git a/Heter_paper.tex b/Heter_paper.tex
index 2b32358..af3d660 100644
--- a/Heter_paper.tex
+++ b/Heter_paper.tex
@@ -88,9 +88,10 @@ platforms many techniques have been  used. Dynamic voltage and frequency scaling
 consumption.  However,  lowering the  frequency  of  a  CPU might  increase  the
 execution  time of  an application  running on  that processor.   Therefore, the
 frequency that  gives the best trade-off  between the energy  consumption and the
-performance of an application must be selected.\\
-In this  paper, a new  online frequencies selecting algorithm  for heterogeneous
-platforms is presented.   It selects the frequency which tries  to give the best
+performance of an application must be selected.
+
+In this  paper, a new  online frequency selecting algorithm  for heterogeneous
+platforms is presented.   It selects the frequencies and tries  to give the best
 trade-off  between  energy saving  and  performance  degradation,  for each  node
 computing the message  passing iterative application. The algorithm  has a small
 overhead and works without training or profiling. It uses a new energy model for
