X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/mpi-energy2.git/blobdiff_plain/bb34e519a34c0aaf166689c6d35ddfd4dc3a318f..b5223cc9bb4a6405c85af04a40e513070c16a235:/Heter_paper.tex

diff --git a/Heter_paper.tex b/Heter_paper.tex
index 069021b..274cf85 100644
--- a/Heter_paper.tex
+++ b/Heter_paper.tex
@@ -903,7 +903,7 @@ down the frequencies of some nodes have less effect on the performance.
 
 
 \subsection{The results for different power consumption scenarios}
-
+\label{sec.compare}
 The results of the previous section were obtained while using processors that consume during computation 
 an overall power which is 80\% composed of  dynamic power and 20\% of static power. In this section, 
 these ratios are changed and two new power scenarios are considered in order to evaluate how the proposed  
@@ -1033,15 +1033,29 @@ for a heterogeneous cluster composed of four different types of nodes having the
 table~(\ref{table:platform}), it takes on average \np[ms]{0.04}  for 4 nodes and \np[ms]{0.15} on average for 144 nodes 
 to compute the best scaling factors vector.  The algorithm complexity is $O(F\cdot (N \cdot4) )$, where $F$ is the number 
 of iterations and $N$ is the number of computing nodes. The algorithm needs  from 12 to 20 iterations to select the best 
-vector of frequency scaling factors that gives the results of the section (\ref{sec.res}).
+vector of frequency scaling factors that gives the results of the sections (\ref{sec.res}) and (\ref{sec.compare}) .
 
 \section{Conclusion}
 \label{sec.concl}
-
+In this paper, we have presented a new online heterogeneous scaling algorithm
+that selects the best possible vector of frequency scaling factors. This vector 
+gives the maximum distance (optimal tradeoff) between the normalized energy and 
+the performance curves. In addition, we developed a new energy model for measuring  
+and predicting the energy of distributed iterative applications running over heterogeneous 
+cluster. The proposed method evaluated on Simgrid/SMPI  simulator to built a heterogeneous 
+platform to executes NAS parallel benchmarks. The results of the experiments showed the ability of
+the proposed algorithm to changes its behaviour to selects different scaling factors  when 
+the number of computing nodes and both of the static and the dynamic powers are changed. 
+
+In the future, we plan to improve this method to apply on asynchronous  iterative applications 
+where each task does not wait the others tasks to finish there works. This leads us to develop a new 
+energy model to an asynchronous iterative applications, where the number of iterations is not 
+known in advance and depends on the global convergence of the iterative system.
 
 \section*{Acknowledgment}
 
 
+
 % trigger a \newpage just before the given reference
 % number - used to balance the columns on the last page
 % adjust value as needed - may need to be readjusted if
