X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/mpi-energy2.git/blobdiff_plain/c21fdc56ee3f50369bfd1f4fcb5caa5c4255a570..7c598f9d3894ffc00d894cfcbd7684d51fb7c14a:/Heter_paper.tex?ds=sidebyside

diff --git a/Heter_paper.tex b/Heter_paper.tex
index 4689caf..6be3c9f 100644
--- a/Heter_paper.tex
+++ b/Heter_paper.tex
@@ -981,7 +981,7 @@ significantly reduces the energy consumption (up to \np[\%]{35}) and tries to
 limit the performance degradation.  They also show that the energy saving
 percentage decreases when the number of computing nodes increases.  This
 reduction is due to the increase of the communication times compared to the
-execution times when the benchmarks are run over a high number of nodes.
+execution times when the benchmarks are run over a higher number of nodes.
 Indeed, the benchmarks with the same class, C, are executed on different numbers
 of nodes, so the computation required for each iteration is divided by the
 number of computing nodes.  On the other hand, more communications are required
