X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/mpi-energy2.git/blobdiff_plain/e11cd9c26d47da75e3ff6ac3e218f644ea6e5314..bccd2d6b1e21a38a16b40d706349b390291ee9f0:/Heter_paper.tex

diff --git a/Heter_paper.tex b/Heter_paper.tex
index 390b151..52883a3 100644
--- a/Heter_paper.tex
+++ b/Heter_paper.tex
@@ -90,7 +90,7 @@ works without training or profiling. It uses a new energy model for message pass
 running on a heterogeneous platform. The proposed algorithm is evaluated  on the Simgrid simulator while 
 running the NAS parallel benchmarks. The experiments demonstrated that it reduces the energy consumption 
 up to 35\% while limiting the performance degradation as much as possible. \textcolor{red}{Furthermore, we compare the
-proposed algorithm with other method. The comparisonâs results show that our algorithm gives better
+proposed algorithm with other method. The comparison results show that our algorithm gives better
 energy-time trade-off.}
 
 \end{abstract}
