X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/mpi-energy2.git/blobdiff_plain/e25948dd52ceacdc4dc6175e899ae810ea4cc134..31b2783760f2dd690f2bade6d15a67fbb2252c22:/Heter_paper.tex?ds=inline

diff --git a/Heter_paper.tex b/Heter_paper.tex
index 90793bf..5b6e349 100644
--- a/Heter_paper.tex
+++ b/Heter_paper.tex
@@ -260,7 +260,7 @@ where $TcpOld_i$ is the computation time  of processor $i$ during the first
 iteration and $MinTcm$ is the communication time of the slowest processor from 
 the first iteration.  The model computes the maximum computation time 
 with scaling factor from each node  added to the communication time of the \subsection{The verifications of the proposed method}
-\label{sec.verif}
+\label{sec.verif.method}
 The precision of the proposed algorithm mainly depends on the execution time prediction model defined in 
 EQ(\ref{eq:perf}) and the energy model computed by EQ(\ref{eq:energy}). 
 The energy model is also significantly dependent  on the execution time model because the static energy is 
@@ -638,7 +638,7 @@ which results in bigger energy savings.
 \end{algorithm}
 
 \subsection{The verifications of the proposed algorithm}
-\label{sec.verif}
+\label{sec.verif.algo}
 The precision of the proposed algorithm mainly depends on the execution time prediction model defined in 
 EQ(\ref{eq:perf}) and the energy model computed by EQ(\ref{eq:energy}). 
 The energy model is also significantly dependent  on the execution time model because the static energy is 
