X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/mpi-energy2.git/blobdiff_plain/ee26b603924e0c91a3e8bfda8acb626fe1502394..cdc55cc9fb92c0969e7c5773567fad0348c8a6dc:/Heter_paper.tex?ds=sidebyside

diff --git a/Heter_paper.tex b/Heter_paper.tex
index c48c927..0b545e4 100644
--- a/Heter_paper.tex
+++ b/Heter_paper.tex
@@ -41,26 +41,17 @@
 \newcommand{\MaxDist}{\mathit{Max}\Dist}
 \newcommand{\MinTcm}{\mathit{Min}\Tcm}
 \newcommand{\Ntrans}{\Xsub{N}{trans}}
+\newcommand{\Pd}{\Xsub{P}{d}}
 \newcommand{\PdNew}{\Xsub{P}{dNew}}
 \newcommand{\PdOld}{\Xsub{P}{dOld}}
-%\newcommand{\Pdyn}{\Xsub{P}{dyn}}
-\newcommand{\Pd}{\Xsub{P}{d}}
-%\newcommand{\PnormInv}{\Xsub{P}{NormInv}}
 \newcommand{\Pnorm}{\Xsub{P}{Norm}}
-%\newcommand{\Pstates}{\Xsub{P}{states}}
-%\newcommand{\Pstatic}{\Xsub{P}{static}}
 \newcommand{\Ps}{\Xsub{P}{s}}
 \newcommand{\Scp}{\Xsub{S}{cp}}
 \newcommand{\Sopt}{\Xsub{S}{opt}}
 \newcommand{\Tcm}{\Xsub{T}{cm}}
-%\newcommand{\Tcomp}{\Xsub{T}{comp}}
-\newcommand{\TcpOld}{\Xsub{T}{cpOld}}
 \newcommand{\Tcp}{\Xsub{T}{cp}}
-%\newcommand{\TmaxCommOld}{\Xsub{T}{Max Comm Old}}
-%\newcommand{\TmaxCompOld}{\Xsub{T}{Max Comp Old}}
-%\newcommand{\Tmax}{\Xsub{T}{max}}
+\newcommand{\TcpOld}{\Xsub{T}{cpOld}}
 \newcommand{\Tnew}{\Xsub{T}{New}}
-%\newcommand{\Tnorm}{\Xsub{T}{Norm}}
 \newcommand{\Told}{\Xsub{T}{Old}} 
 
 \begin{document} 
@@ -1139,6 +1130,24 @@ degradation.
   \label{table:res_s2}
 \end{table}
 
+\begin{table}[!t]
+ \caption{Comparing the proposed algorithm}
+ \centering
+\begin{tabular}{|*{7}{r|}}
+\hline
+Program & \multicolumn{2}{c|}{Energy saving \%} & \multicolumn{2}{c|}{Perf.  degradation \%} & \multicolumn{2}{c|}{Distance} \\ \cline{2-7} 
+name    & EDP             & MaxDist          & EDP            & MaxDist           & EDP          & MaxDist        \\ \hline
+CG      & 27.58           & 31.25            & 5.82           & 7.12              & 21.76        & 24.13          \\ \hline
+MG      & 29.49           & 33.78            & 3.74           & 6.41              & 25.75        & 27.37          \\ \hline
+LU      & 19.55           & 28.33            & 0.0            & 0.01              & 19.55        & 28.22          \\ \hline
+EP      & 28.40           & 27.04            & 4.29           & 0.49              & 24.11        & 26.55          \\ \hline
+BT      & 27.68           & 32.32            & 6.45           & 7.87              & 21.23        & 24.43          \\ \hline
+SP      & 20.52           & 24.73            & 5.21           & 2.78              & 15.31         & 21.95         \\ \hline
+FT      & 27.03           & 31.02            & 2.75           & 2.54              & 24.28        & 28.48           \\ \hline
+
+\end{tabular}
+\label{table:compare_EDP}
+\end{table}
 
 \begin{figure}[!t]
   \centering
@@ -1151,7 +1160,12 @@ degradation.
   \caption{The comparison of the three power scenarios}
 \end{figure}  
 
-
+\begin{figure}[!t]
+  \centering
+   \includegraphics[scale=0.5]{fig/compare_EDP.pdf}
+  \caption{Trade-off comparison for NAS benchmarks class C}
+  \label{fig:compare_EDP}
+\end{figure}
 
 
 \subsection{The comparison of the proposed scaling algorithm }
@@ -1188,39 +1202,6 @@ because it maximizes the distance  between the energy saving and the performance
 degradation values while giving the same weight for both metrics.
 
 
-
-
-\begin{table}[!t]
- \caption{Comparing the proposed algorithm}
- \centering
-\begin{tabular}{|*{7}{r|}}
-\hline
-Program & \multicolumn{2}{c|}{Energy saving \%} & \multicolumn{2}{c|}{Perf.  degradation \%} & \multicolumn{2}{c|}{Distance} \\ \cline{2-7} 
-name    & EDP             & MaxDist          & EDP            & MaxDist           & EDP          & MaxDist        \\ \hline
-CG      & 27.58           & 31.25            & 5.82           & 7.12              & 21.76        & 24.13          \\ \hline
-MG      & 29.49           & 33.78            & 3.74           & 6.41              & 25.75        & 27.37          \\ \hline
-LU      & 19.55           & 28.33            & 0.0            & 0.01              & 19.55        & 28.22          \\ \hline
-EP      & 28.40           & 27.04            & 4.29           & 0.49              & 24.11        & 26.55          \\ \hline
-BT      & 27.68           & 32.32            & 6.45           & 7.87              & 21.23        & 24.43          \\ \hline
-SP      & 20.52           & 24.73            & 5.21           & 2.78              & 15.31         & 21.95         \\ \hline
-FT      & 27.03           & 31.02            & 2.75           & 2.54              & 24.28        & 28.48           \\ \hline
-
-\end{tabular}
-\label{table:compare_EDP}
-\end{table}
-
-
-
-
-
-\begin{figure}[!t]
-  \centering
-   \includegraphics[scale=0.5]{fig/compare_EDP.pdf}
-  \caption{Trade-off comparison for NAS benchmarks class C}
-  \label{fig:compare_EDP}
-\end{figure}
-
-
 \section{Conclusion}
 \label{sec.concl} 
 In this paper, a new online frequency selecting algorithm has been presented. It
