X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/mpi-energy2.git/blobdiff_plain/f4ce4e7c41e562ada4beac5e59c39a2db86a902f..cd337b2e1390f7825113c221be31c1d9ecf55c98:/Heter_paper.tex?ds=sidebyside

diff --git a/Heter_paper.tex b/Heter_paper.tex
index a1f6b22..6a62dfd 100644
--- a/Heter_paper.tex
+++ b/Heter_paper.tex
@@ -692,7 +692,7 @@ The results of the previous section are obtained using a percentage of 80\% for
   \quad%
   \subfloat[Comparison the selected frequency scaling factors for 8 nodes]{%
     \includegraphics[width=.24\textwidth]{fig/three_scenarios}\label{fig:scales_comp}}
-  \label{fig:avg}
+  \label{fig:comp}
   \caption{The comparison of the three power scenarios}
 \end{figure}
 
