X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/Sensornets15.git/blobdiff_plain/9bc38095022b21c8005ea6af50223a60ace36718..5442cc8a9128527983d0c1f0f7259531eca9330b:/reponse.tex?ds=inline

diff --git a/reponse.tex b/reponse.tex
index 8a70d92..9b38abb 100644
--- a/reponse.tex
+++ b/reponse.tex
@@ -73,8 +73,8 @@ the comments and the revision for the original manuscript.
 
 The paper present a new system to optimize sensord detections. The work present the algorithm in a cleare and well descrived way. The main problem is connected with the luck of examples and also on the practical applications. I suggest in future to make a more formal description of the process.\\
 \textcolor{blue}{\textbf{\textsc{Answer:} Right. We have included  a paragraph on examples and  practical applications of  WSNs in section~1.}}
-\textcolor{red}{Je pense que la question porte sur un exemple d'application de notre protocole?}
-\textcolor{magenta}{Je pense que oui.}
+%\textcolor{red}{Je pense que la question porte sur un exemple d'application de notre protocole?}
+%\textcolor{magenta}{Je pense que oui.}
 
 \section*{Response to Reviewer $\#$3 Comments}
 
@@ -83,9 +83,9 @@ This work proposed a distributed lifetime coverage optimization (DiLCO) protocol
 \textcolor{blue}{\textbf{\textsc{Answer:}
 %The difference between our leader selection technique and the methods of cluster head election in LEACH or other distributed protocols in that our approach  assumes  that the sensors are deployed almost uniformly and with high density over the region. So we only need  to fix a regular division of the  region into subregions to make the problem tractable.  The subdivision is made using divide-and-conquer concept such that the number of hops between any pairs  of sensors inside a subregion is  less than or equal to~3. The sensors inside each subregion cooperate to elect one leader. Leader applies sensor activity scheduling based optimization to provide the schedule to the sensor nodes in the subregion. The advantage of our approach is to minimize the energy consumption required for communication. The sensors only require to communicate with the other sensors inside the subregion to elect the leader instead of communicating with other nodes in the WSN. \\Whereas in LEACH and other cluster head election methods, the cluster heads are elected in distributed way where sensors  elect  themselves  to  be local cluster-heads  at any  given time  with  a  certain  probability. These cluster-head  nodes  broadcast  their  status  to  the  other  sensors  in the network.  Each sensor node determines to which cluster it wants to belong by choosing the cluster-head that requires the minimum communication energy. Once all the nodes are organized into clusters, each cluster-head creates a schedule for the nodes in its cluster.   \\\\
     In our  approach, the leader selection technique is quite different from the LEACH protocol or from its variants. Contrary to the LEACH protocol, the division of the area of interest into subregions is assumed to be performed before the head election. Moreover, we assume that sensors are deployed almost uniformly and with high density over the area of interest, such that the division is fixed and regular. As in LEACH, our protocol works in round fashion. In each round, during the pre-sensing phase, nodes make autonomous decisions. In LEACH, each sensor elects itself to be a cluster head, and each non-cluster head will determine its cluster for the round. In our protocol, nodes in the same subregion select their leader. In both protocols, the amount of remaining energy in each  node is taken into account to promote the nodes that have the most energy to become leader. Contrary to the LEACH protocol where all sensors will be active during the sensing-phase, our protocol allows to deactivate a subset of sensors through an optimization process which reduces significantly the energy consumption.\\\\
-As explained by the reviewer, there is a large variety of energy-efficient protocols for WSN. We focus on GAF and DESK protocols for two main reasons. First, our protocol is inspired by both of them. DiLCO uses a regular division of the area as in GAF protocol and a temporal division in rounds as in DESK. Second,  GAF and DESK are well-known protocols, easy to implement, and often used as references for comparison. \textcolor{red}{je ne sais pas si on ne devrait pas inclure une ref \`a LEACH dans la biblio, mais je ne sais pas trop comment l'introduire dans le papier...}
-\textcolor{magenta}{Le premier paragraphe de ta r\'eponse me semble pas mal, juste pour situer notre protocole par rapport à LEACH. On pourrait le mettre dans la section~2 ?}\\\\ }}
-%In fact, GAF algorithm is chosen for comparison as a competitor because it is famous and easy to implement, as well as many authors referred to it in many publications. DESK algorithm is also selected as competitor in the comparison because it works into rounds fashion (network lifetime divided into rounds) similar to our approaches, as well as DESK is a full distributed coverage approach. }}
+As explained by the reviewer, there is a large variety of energy-efficient protocols for WSN. We focus on GAF and DESK protocols for two main reasons. First, our protocol is inspired by both of them. DiLCO uses a regular division of the area as in GAF protocol and a temporal division in rounds as in DESK. Second,  GAF and DESK are well-known protocols, easy to implement, and often used as references for comparison.}} %\textcolor{red}{je ne sais pas si on ne devrait pas inclure une ref \`a LEACH dans la biblio, mais je ne sais pas trop comment l'introduire dans le papier...}
+%\textcolor{magenta}{Le premier paragraphe de ta r\'eponse me semble pas mal, juste pour situer notre protocole par rapport à LEACH. On pourrait le mettre dans la section~2 ?}\\\\ }}
+%In fact, GAF algorithm is chosen for comparison as a competitor because it is famous and easy to implement, as well as many authors referred to it in many publications. DESK algorithm is also selected as competitor in the comparison because it works into rounds fashion (network lifetime divided into rounds) similar to our approaches, as well as DESK is a full distributed coverage approach.}}
 
 \noindent The following improvements may be suggested to make it even better:\\
 \noindent {\bf 1. What is the ``new idea" or contribution of this work?}\\
