X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/28fe5f530e0e9ae044a4463fd7eb3646cc5dd04c..5c431ecbeda4acd97fad6b1e170d502ea11a2b3d:/CHAPITRE_03.tex

diff --git a/CHAPITRE_03.tex b/CHAPITRE_03.tex
index a4dd3fa..93b3b3b 100644
--- a/CHAPITRE_03.tex
+++ b/CHAPITRE_03.tex
@@ -112,7 +112,7 @@ OMNeT++ (Objective Modular Network Testbed) is an open-source, free, discrete-ev
 
 \item \textbf{OPNET:}
 
-OPNET (Optimized Network Engineering tool)~\cite{ref192,ref200,ref201} is the first commercial simulation tool developed in 1987 for communication networks. It is a discrete event, object-oriented, general purpose network simulator, which is widely used in industry. It uses C and Java languages. It provides a comprehensive development environment for the specification, simulation, configuration, and performance analysis of the communication network. OPNET allows researchers to develop various models by means of a graphical interface. It provides different types of tools such as Probe Editor, Filter Tool, and Animation Viewer for data collection to model graph and animate the resulting output. Unlike ns-2, OPNET provides modeling for different sensor-specific hardware, such as physical-link transceivers and antennas. It includes sensor-specific models such as ad-hoc connectivity, mobility of nodes, node failure models, modeling of power-consumption, etc. OPNET is, a commercial simulator and the license is very expensive. This represents the main disadvantage of that simulator.
+OPNET (Optimized Network Engineering Tool)~\cite{ref192,ref200,ref201} is the first commercial simulation tool developed in 1987 for communication networks. It is a discrete event, object-oriented, general purpose network simulator, which is widely used in industry. It uses C and Java languages. It provides a comprehensive development environment for the specification, simulation, configuration, and performance analysis of the communication network. OPNET allows researchers to develop various models by means of a graphical interface. It provides different types of tools such as Probe Editor, Filter Tool, and Animation Viewer for data collection to model graph and animate the resulting output. Unlike ns-2, OPNET provides modeling for different sensor-specific hardware, such as physical-link transceivers and antennas. It includes sensor-specific models such as ad-hoc connectivity, mobility of nodes, node failure models, modeling of power-consumption, etc. OPNET is, a commercial simulator and the license is very expensive. This represents the main disadvantage of that simulator.
 
 
 \item \textbf{GloMoSim:} 
