X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/28fe5f530e0e9ae044a4463fd7eb3646cc5dd04c..6d401cb266bc54619b552e898e3717db5c4b4f59:/CHAPITRE_06.tex?ds=inline

diff --git a/CHAPITRE_06.tex b/CHAPITRE_06.tex
index bd0cdf8..121ae35 100644
--- a/CHAPITRE_06.tex
+++ b/CHAPITRE_06.tex
@@ -86,7 +86,7 @@ obtained through  the formula: $$\alpha =  \arccos \left(\dfrac{Dist(u,v)}{2R_s}
 Every couple of intersection points is placed on the angular interval $[0,2\pi]$
 in  a  counterclockwise manner,  leading  to  a  partitioning of  the  interval.
 Figure~\ref{pcm2sensors}(a)  illustrates  the arcs  for  the  nine neighbors  of
-sensor $0$ and  Figure~\ref{expcm} gives the position of  the corresponding arcs
+sensor $0$ and  Figure~\ref{expcm} gives the position of the corresponding arcs
 in  the interval  $[0,2\pi]$. More  precisely, we  can see  that the  points are
 ordered according  to the  measures of  the angles  defined by  their respective
 positions. The intersection points are  then visited one after another, starting
