<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">X-Git-Url: https://bilbo.iut-bm.univ-fcomte.fr/and/gitweb/ThesisAli.git/blobdiff_plain/81197a19a27249d75ca25536fab51cfbd68176b8..471e797ea207eea3a79a42ef48e6c3b14f3c004b:/CHAPITRE_01.tex?ds=sidebyside

diff --git a/CHAPITRE_01.tex b/CHAPITRE_01.tex
index 7459496..ddc551c 100644
--- a/CHAPITRE_01.tex
+++ b/CHAPITRE_01.tex
@@ -116,7 +116,7 @@ This kind of WSN consists of low-cost wireless sensor nodes, which are embedded
 \section{Applications}
 \label{ch1:sec:04}
 %\indent The fast development in WSNs has been led to study  their different characteristics extensively. However, the WSN is concentrated on various applications. 
-In this section, we describe different academic and commercial applications. A WSN can use various types of sensors such as \cite{ref17,ref19}: thermal, seismic, magnetic, visual, infrared, acoustic, and radar. These sensors are capable of observing a different physical conditions such as: temperature, humidity, pressure, speed, direction, movement, light, soil makeup, noise levels, presence or absence of certain kinds of objects, and mechanical stress levels on attached objects. Consequently, a wide range of WSN applications can be classified into five classes~\cite{ref22}, as shown in Figure~\ref{WSNAP}. 
+In this section, we describe different academic and commercial applications. A WSN can use various types of sensors such as \cite{ref17,ref19}: thermal, seismic, magnetic, visual, infrared, acoustic, and radar. These sensors are capable of observing  different physical conditions such as: temperature, humidity, pressure, speed, direction, movement, light, soil makeup, noise levels, presence or absence of certain kinds of objects, and mechanical stress levels on attached objects. Consequently, a wide range of WSN applications can be classified into five classes~\cite{ref22}, as shown in Figure~\ref{WSNAP}. 
 
 \begin{figure}[h!]
 \centering
</pre></body></html>